9.0 Charging tool
On the (6.0.3) fast charge identification page, long- click the right button
to enter the charging tool menu. The functions are:
1 PD monitor.
2 Read the E-Marker cable.
3 Read the DASH cable.
4 Analog DASH cable.
5 Apple 2.4A acceleration.
9.0.1 PD Listener
When using PD listener,Need to turn the PD communication switch to
ON,And use a power supply not greater than 16V (usually 5V) and a Micro
-USB cable,Connect the PC online port,Provide external power.
Use the PD listener function,Need 2 C-C cables,Connect the charger
and PD electrical appliances from the Type-CIN interface and Type-COUT
interface respectively.When the connection is normal and the PD protocol
triggered by the PD consumer is captured,The page is represented as
shown below.When the PD charger cannot be powered,Because the C-C cable
has only one-sided CC,And the 2 CCs are not connected,So you can flip
one of the C-C cable connectors,Solve the problem.
The figure below,The charger is a 65W PD charging head,The current
PD appliance chooses the third gear,Trigger the target voltage
12V,Maximum current 3A.
23