10.3.1 Trigger time
Set trigger time.
10.3.2 Block PD CDC
After opening,When PD is monitoring,CRC messages can be masked,Off by
default.
10.3.2 Boot simulation DASH
After it is turned on, turn on the analog DASH cable function at boot,
which is turned off by default.
10.3.2 Boot Apple 2.4A
After opening,Turn on the Apple 2.4A acceleration function when booting,
Off by default.
10.4 Settings menu -> system
You can view information such as the operating times of the instrument,
SN serial number, and software version.
11.0 Upgrade firmware instructions
1 Open the FNIRSIUSBMeter upgrade tool.
2 When the meter is off, press the middle button to access
the PC online port, it will display the connected, device
model, and device firmware version.
3 Click OPEN and choose to upgrade the firmware.
4 Click START to start the firmware upgrade. After the
upgrade is completed, the meter will automatically restart
and enter the main interface.
28