8.0.1 Fast charge protocol automatic detection
In this mode,The meter tries to trigger various protocols in
turn,Display the test results on the screen,Red is not supported,Green is
support,In the process of testing,Such as measuring PD chargers,It is
normal to restart and continue testing.During the test, it is forbidden to
connect to any equipment at the back end.
It does not respond to any key operation during the test. If you want
to exit during the test, please unplug the meter directly. After the test
is completed, click the middle button to start the test again; click the
BACK button to return to the previous page.
8.0.2 QC2.0 Trigger
In QC2.0 trigger mode, use the left and right keys to select the trigger
voltage, and click BACK to return.
19