4
PD2.0/3.0 Trigger;
5
VOOC/WARP Trigger;
6
SuperVOOC Trigger;
7
The above protocols all support automatic monitoring
MTK-PE automatic detection;
Support QC2.0->PD2.0 protocol conversion;
8
9
10
Support a maximum of 24 hours for a limited time trigger, and
automatically close the trigger when the time comes
3.0.5 Wire identification class
1
2
3
The internal resistance measurement of the wire by the differential pressure method;
E-Marker Cable chip reading;
DASH Cable data reading;
3.0.5 Miscellaneous
1 Record of startup time;
2 Onboard temperature measurement;
3 Gravity sensor, automatically switch the display direction;
4 PD monitor;
5 Analog DASH cable;
6 Apple 2.4A acceleration;
6