# Static Call Graph for image ..\OBJ\WKS35WQV001.axf

#<CALLGRAPH># ARM Linker, 5060300: Last Updated: Fri May 17 19:14:02 2019

### Maximum Stack Usage = 416 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ GT9147_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FPU_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PVD_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RCC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - Reset_Handler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f40_41xxx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TP_Adjust from touch.o(.text) referenced from touch.o(.data)
  - TP_Init from touch.o(.text) referenced from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f40_41xxx.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_hex

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_string

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 416 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ GT9147_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Load_Drow_Dialog (Thumb, 64 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Load_Drow_Dialog ⇒ LT738_Print_Internal_Font_String ⇒ Goto_Text_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LT738_Select_Internal_Font_Init
  - >> LT738_Print_Internal_Font_String
  - >> LT738_DrawSquare_Fill
  [Called By]
  - >> main
  - >> ctp_test

  lcd_draw_bline (Thumb, 212 bytes, Stack size 72 bytes, main.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = lcd_draw_bline ⇒ LT738_DrawCircle_Fill ⇒ Circle_Center_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LT738_DrawCircle_Fill
  [Called By]
  - >> ctp_test

  ctp_test (Thumb, 294 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = ctp_test ⇒ GT9147_Scan ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> GT9147_Scan
  - >> lcd_draw_bline
  - >> Load_Drow_Dialog
  [Called By]
  - >> main

  main (Thumb, 642 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 416 + Unknown Stack Size
  - Call Chain = main ⇒ GT9147_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> uart_init
  - >> delay_ms
  - >> delay_init
  - >> WaitKey
  - >> WB_block
  - >> Select_Main_Window_16bpp
  - >> Parallel_Init
  - >> NVIC_PriorityGroupConfig
  - >> Main_Window_Start_XY
  - >> Main_Image_Width
  - >> Main_Image_Start_Address
  - >> LT738_Select_Internal_Font_Init
  - >> LT738_Print_Internal_Font_String
  - >> LT738_PWM1_Init
  - >> LT738_Init
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawCircle
  - >> LED_Init
  - >> KEY_Init
  - >> GT9147_Init
  - >> GRAY_32
  - >> Display_picture
  - >> Display_ON
  - >> Delay_ms
  - >> Canvas_image_width
  - >> Canvas_Image_Start_address
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> ctp_test
  - >> Load_Drow_Dialog
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(.text)

  SystemCoreClockUpdate (Thumb, 174 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  LED_Init (Thumb, 60 bytes, Stack size 16 bytes, led.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Init (Thumb, 60 bytes, Stack size 16 bytes, key.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  Scan_Key (Thumb, 100 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> Scan_FunctionKey
  - >> Scan_Key_delay
  - >> Waiting_Key

  Waiting_Key (Thumb, 20 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> Scan_Key

  WaitKey (Thumb, 30 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = WaitKey ⇒ delay_ms
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> main
  - >> Show

  WaitKeyBL (Thumb, 30 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> delay_ms

  Scan_Key_delay (Thumb, 50 bytes, Stack size 16 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> Scan_Key
  - >> delay_ms

  Scan_FunctionKey (Thumb, 156 bytes, Stack size 24 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> Scan_Key
  - >> delay_ms

  KEY_Scan (Thumb, 188 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> delay_ms

  Delay_us (Thumb, 30 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> Enable_PLL
  - >> LT738_PLL_Initial

  Delay_ms (Thumb, 32 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> LT738_Init
  - >> main
  - >> LT738_SDRAM_initail
  - >> LT738_PLL_Initial
  - >> System_Check_Temp
  - >> LT738_HW_Reset

  FSMC_IO_Init (Thumb, 562 bytes, Stack size 136 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = FSMC_IO_Init ⇒ GPIO_PinAFConfig
  [Calls]
  - >> RCC_AHB3PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> Parallel_Init

  FMSC_16_CmdWrite (Thumb, 6 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> LCD_CmdWrite

  FMSC_16_DataWrite (Thumb, 8 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> LCD_DataWrite

  FMSC_16_DataWrite_Pixel (Thumb, 8 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> LCD_DataWrite_Pixel

  FMSC_16_StatusRead (Thumb, 10 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> LCD_StatusRead

  FMSC_16_DataRead (Thumb, 10 bytes, Stack size 0 bytes, if_port.o(.text), UNUSED)

  LCD_CmdWrite (Thumb, 12 bytes, Stack size 4 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_CmdWrite
  [Calls]
  - >> FMSC_16_CmdWrite
  [Called By]
  - >> LCD_VSYNC_Pulse_Width
  - >> LCD_VSYNC_Start_Position
  - >> LCD_Vertical_Non_Display
  - >> LCD_HSYNC_Pulse_Width
  - >> LCD_HSYNC_Start_Position
  - >> LCD_Horizontal_Non_Display
  - >> LCD_HorizontalWidth_VerticalHeight
  - >> Idle_VSYNC_High
  - >> Idle_VSYNC_Low
  - >> Idle_HSYNC_High
  - >> Idle_HSYNC_Low
  - >> Idle_PDAT_High
  - >> Idle_PDAT_Low
  - >> Idle_PCLK_High
  - >> Idle_PCLK_Low
  - >> Idle_DE_High
  - >> Idle_DE_Low
  - >> DE_High_Active
  - >> DE_Low_Active
  - >> VSYNC_High_Active
  - >> VSYNC_Low_Active
  - >> HSYNC_High_Active
  - >> HSYNC_Low_Active
  - >> PDATA_IDLE_STATE
  - >> PDATA_Set_BGR
  - >> PDATA_Set_BRG
  - >> PDATA_Set_GBR
  - >> PDATA_Set_GRB
  - >> PDATA_Set_RBG
  - >> PDATA_Set_RGB
  - >> VSCAN_B_to_T
  - >> VSCAN_T_to_B
  - >> HSCAN_R_to_L
  - >> HSCAN_L_to_R
  - >> Color_Bar_OFF
  - >> Color_Bar_ON
  - >> Display_OFF
  - >> PCLK_Falling
  - >> PCLK_Rising
  - >> Select_PIP1_Window_24bpp
  - >> Select_PIP1_Window_16bpp
  - >> Select_PIP1_Window_8bpp
  - >> Select_PIP2_Window_24bpp
  - >> Select_PIP2_Window_16bpp
  - >> Select_PIP2_Window_8bpp
  - >> Select_Main_Window_24bpp
  - >> Select_Main_Window_8bpp
  - >> Select_PIP2_Parameter
  - >> Select_PIP1_Parameter
  - >> Disable_PIP2
  - >> Enable_PIP2
  - >> Disable_PIP1
  - >> Enable_PIP1
  - >> XPDAT0_Set_KIN1
  - >> XPDAT0_Set_GPIO_D0
  - >> XPDAT1_Set_KIN2
  - >> XPDAT1_Set_GPIO_D1
  - >> XPDAT2_Set_KIN4
  - >> XPDAT2_Set_GPIO_D6
  - >> XPDAT8_Set_KIN3
  - >> XPDAT8_Set_GPIO_D2
  - >> XPDAT9_Set_KOUT3
  - >> XPDAT9_Set_GPIO_D3
  - >> XPDAT16_Set_KOUT1
  - >> XPDAT16_Set_GPIO_D4
  - >> XPDAT17_Set_KOUT2
  - >> XPDAT17_Set_GPIO_D5
  - >> XPDAT18_Set_KOUT4
  - >> XPDAT18_Set_GPIO_D7
  - >> Disable_XDB7_0_PullUp
  - >> Disable_XDB15_8_PullUp
  - >> Disable_GPIOC_PullUp
  - >> Disable_GPIOD_PullUp
  - >> Disable_GPIOE_PullUp
  - >> Disable_GPIOF_PullUp
  - >> Enable_XDB7_0_PullUp
  - >> Enable_XDB15_8_PullUp
  - >> Enable_GPIOC_PullUp
  - >> Enable_GPIOD_PullUp
  - >> Enable_GPIOE_PullUp
  - >> Enable_GPIOF_PullUp
  - >> Enable_PWM0_Interrupt_Flag
  - >> Enable_PWM1_Interrupt_Flag
  - >> Enable_Draw_BTE_Interrupt_Flag
  - >> Enable_KeyScan_Interrupt_Flag
  - >> Enable_Vsync_Interrupt_Flag
  - >> Enable_I2CM_Interrupt_Flag
  - >> Enable_ExtInterrupt_Inpur_Flag
  - >> Enable_Resume_Interrupt_Flag
  - >> Mask_PWM0_Interrupt_Flag
  - >> Mask_PWM1_Interrupt_Flag
  - >> Mask_Draw_BTE_Interrupt_Flag
  - >> Mask_KeyScan_Interrupt_Flag
  - >> Mask_Vsync_Interrupt_Flag
  - >> Mask_I2CM_Interrupt_Flag
  - >> Mask_ExtInterrupt_Input_Flag
  - >> Mask_Resume_Interrupt_Flag
  - >> Clear_PWM0_Interrupt_Flag
  - >> Clear_PWM1_Interrupt_Flag
  - >> Clear_Draw_BTE_Interrupt_Flag
  - >> Clear_KeyScan_Interrupt_Flag
  - >> Clear_Vsync_Interrupt_Flag
  - >> Clear_I2CM_Interrupt_Flag
  - >> Clear_ExtInterrupt_Input_Flag
  - >> Clear_Resume_Interrupt_Flag
  - >> Read_Interrupt_status
  - >> Disable_PWM0_Interrupt
  - >> Enable_PWM0_Interrupt
  - >> Disable_PWM1_Interrupt
  - >> Enable_PWM1_Interrupt
  - >> Disable_DMA_Draw_BTE_Interrupt
  - >> Enable_DMA_Draw_BTE_Interrupt
  - >> Disable_KeyScan_Interrupt
  - >> Enable_KeyScan_Interrupt
  - >> Disable_Vsync_Interrupt
  - >> Enable_Vsync_Interrupt
  - >> Disable_I2CM_Interrupt
  - >> Enable_I2CM_Interrupt
  - >> Disable_ExtInterrupt_Input
  - >> Enable_ExtInterrupt_Input
  - >> Disable_Resume_Interrupt
  - >> Enable_Resume_Interrupt
  - >> Memory_Select_Color_Palette_RAM
  - >> Memory_Select_Graphic_Cursor_RAM
  - >> Memory_Select_SDRAM
  - >> Text_Mode
  - >> Graphic_Mode
  - >> LVDS_Format2
  - >> LVDS_Format1
  - >> ExtInterrupt_Input_Rising_Edge_Trigger
  - >> ExtInterrupt_Input_Falling_Edge_Trigger
  - >> ExtInterrupt_Input_High_Level_Trigger
  - >> ExtInterrupt_Input_Low_Level_Trigger
  - >> ExtInterrupt_Nodebounce
  - >> ExtInterrupt_Debounce
  - >> Interrupt_Active_High
  - >> Interrupt_Active_Low
  - >> MemWrite_Down_Top_Left_Right
  - >> MemWrite_Top_Down_Left_Right
  - >> MemWrite_Right_Left_Top_Down
  - >> MemWrite_Left_Right_Top_Down
  - >> MemRead_Down_Top_Left_Right
  - >> MemRead_Top_Down_Left_Right
  - >> MemRead_Right_Left_Top_Down
  - >> MemRead_Left_Right_Top_Down
  - >> RGB_16b_24bpp_mode2
  - >> RGB_16b_24bpp_mode1
  - >> RGB_16b_16bpp
  - >> RGB_16b_8bpp
  - >> RGB_8b_24bpp
  - >> RGB_8b_16bpp
  - >> RGB_8b_8bpp
  - >> Host_Bus_16bit
  - >> Host_Bus_8bit
  - >> LT738_I2CM_Disable
  - >> LT738_I2CM_Enable
  - >> TFT_LVDS
  - >> TFT_16bit
  - >> TFT_18bit
  - >> TFT_24bit
  - >> Key_Scan_Disable
  - >> Key_Scan_Enable
  - >> LT738_WakeUp
  - >> LT738_Sleep
  - >> Enable_PLL
  - >> LT738_SW_Reset
  - >> LCD_RegisterRead
  - >> LCD_RegisterWrite
  - >> test_FSMCIO
  - >> Select_Main_Window_16bpp
  - >> Display_picture
  - >> Display_ON
  - >> MPU_Memory_Write_Pixel_8bit
  - >> MPU_Memory_Write_Window_8bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_Graphic_cursor_Init
  - >> LT738_Print_Outside_Font_String
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> LT738_PLL_Initial
  - >> System_Check_Temp
  - >> Show_picture
  - >> Show_String
  - >> Read_Key_Strobe_Data_2
  - >> Read_Key_Strobe_Data_1
  - >> Read_Key_Strobe_Data_0
  - >> Numbers_of_Key_Hit
  - >> Long_Key_Timing_Adjustment
  - >> Key_Scan_Wakeup_Function_Enable
  - >> Key_Scan_Freg
  - >> Long_Key_enable
  - >> Read_GPIO_F_7_0
  - >> Write_GPIO_F_7_0
  - >> Set_GPIO_F_In_Out
  - >> Read_GPIO_E_7_0
  - >> Write_GPIO_E_7_0
  - >> Set_GPIO_E_In_Out
  - >> Read_GPIO_D_7_0
  - >> Write_GPIO_D_7_0
  - >> Set_GPIO_D_In_Out
  - >> Read_GPIO_C_7_0
  - >> Write_GPIO_C_7_0
  - >> Set_GPIO_C_In_Out
  - >> Read_GPIO_B_7_0
  - >> Write_GPIO_B_7_4
  - >> Read_GPIO_A_7_0
  - >> Write_GPIO_A_7_0
  - >> Set_GPIO_A_In_Out
  - >> LT738_I2CM_Arbitration
  - >> LT738_I2CM_transmit_Progress
  - >> LT738_I2CM_Bus_Busy
  - >> LT738_I2CM_Check_Slave_ACK
  - >> LT738_I2CM_Write
  - >> LT738_I2CM_Write_With_Start
  - >> LT738_I2CM_Read_With_Nack
  - >> LT738_I2CM_Read_With_Ack
  - >> LT738_I2CM_Stop
  - >> LT738_I2CM_Receiver_Data
  - >> LT738_I2CM_Transmit_Data
  - >> LT738_I2CM_Clock_Prescale
  - >> Power_Saving_Sleep_Mode
  - >> Power_Saving_Suspend_Mode
  - >> Power_Saving_Standby_Mode
  - >> Power_Normal_Mode
  - >> CGRAM_Start_address
  - >> Background_color_16M
  - >> Background_color_65k
  - >> Background_color_256
  - >> Background_RGB
  - >> Foreground_color_16M
  - >> Foreground_color_65k
  - >> Foreground_color_256
  - >> Foreground_RGB
  - >> Set_Font_to_Font_Width
  - >> Font_Line_Distance
  - >> Set_GTFont_Decoder
  - >> GTFont_Select_GT22L16A1Y
  - >> GTFont_Select_GT21L24S1W
  - >> GTFont_Select_GT20L24F6Y
  - >> GTFont_Select_GT23L32S4W_GT23H32S4W
  - >> GTFont_Select_GT23L24M1Z
  - >> GTFont_Select_GT23L24T3Y_GT23H24T3Y
  - >> GTFont_Select_GT23L16U2W
  - >> GTFont_Select_GT21L16TW_GT21H16T1W
  - >> Font_Height_X4
  - >> Font_Height_X3
  - >> Font_Height_X2
  - >> Font_Height_X1
  - >> Font_Width_X4
  - >> Font_Width_X3
  - >> Font_Width_X2
  - >> Font_Width_X1
  - >> Font_90_degree
  - >> Font_0_degree
  - >> Font_Background_select_Color
  - >> Font_Background_select_Transparency
  - >> Disable_Font_Alignment
  - >> Enable_Font_Alignment
  - >> Internal_CGROM_Select_ISOIEC8859_4
  - >> Internal_CGROM_Select_ISOIEC8859_3
  - >> Internal_CGROM_Select_ISOIEC8859_2
  - >> Internal_CGROM_Select_ISOIEC8859_1
  - >> Font_Select_16x32_32x32
  - >> Font_Select_12x24_24x24
  - >> Font_Select_8x16_16x16
  - >> CGROM_Select_Genitop_FontROM
  - >> CGROM_Select_Internal_CGROM
  - >> Font_Select_UserDefine_Mode
  - >> BTE_Alpha_Blending_Effect
  - >> S1_Constant_color_16M
  - >> S1_Constant_color_65k
  - >> S1_Constant_color_256
  - >> BTE_Destination_Color_24bpp
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Destination_Color_8bpp
  - >> BTE_S1_Color_16bit_Alpha
  - >> BTE_S1_Color_8bit_Alpha
  - >> BTE_S1_Color_Constant
  - >> BTE_S1_Color_24bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S1_Color_8bpp
  - >> BTE_S0_Color_24bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_S0_Color_8bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Pattern_Format_16X16
  - >> Pattern_Format_8X8
  - >> BTE_Disable
  - >> BTE_Enable
  - >> Set_Timer1_Count_Buffer
  - >> Set_Timer1_Compare_Buffer
  - >> Set_Timer0_Count_Buffer
  - >> Set_Timer0_Compare_Buffer
  - >> Set_Timer0_Dead_Zone_Length
  - >> Stop_PWM0
  - >> Start_PWM0
  - >> One_Shot_PWM0
  - >> Auto_Reload_PWM0
  - >> Disable_PWM0_Inverter
  - >> Enable_PWM0_Inverter
  - >> Disable_PWM0_Dead_Zone
  - >> Enable_PWM0_Dead_Zone
  - >> Stop_PWM1
  - >> Start_PWM1
  - >> One_Shot_PWM1
  - >> Auto_Reload_PWM1
  - >> Disable_PWM1_Inverter
  - >> Enable_PWM1_Inverter
  - >> Select_PWM0_is_Core_Clock
  - >> Select_PWM0
  - >> Select_PWM0_is_GPIO_C7
  - >> Select_PWM1_is_Osc_Clock
  - >> Select_PWM1
  - >> Select_PWM1_is_ErrorFlag
  - >> Select_PWM0_Clock_Divided_By_8
  - >> Select_PWM0_Clock_Divided_By_4
  - >> Select_PWM0_Clock_Divided_By_2
  - >> Select_PWM0_Clock_Divided_By_1
  - >> Select_PWM1_Clock_Divided_By_8
  - >> Select_PWM1_Clock_Divided_By_4
  - >> Select_PWM1_Clock_Divided_By_2
  - >> Select_PWM1_Clock_Divided_By_1
  - >> Set_PWM_Prescaler_1_to_256
  - >> Circle_Square_Radius_RxRy
  - >> Ellipse_Radius_RxRy
  - >> Circle_Radius_R
  - >> Ellipse_Center_XY
  - >> Circle_Center_XY
  - >> Start_Circle_Square_Fill
  - >> Start_Circle_Square
  - >> Start_Square_Fill
  - >> Start_Square
  - >> Start_Right_Down_Curve_Fill
  - >> Start_Right_Up_Curve_Fill
  - >> Start_Left_Up_Curve_Fill
  - >> Start_Left_Down_Curve_Fill
  - >> Start_Right_Down_Curve
  - >> Start_Right_Up_Curve
  - >> Start_Left_Up_Curve
  - >> Start_Left_Down_Curve
  - >> Start_Circle_or_Ellipse_Fill
  - >> Start_Circle_or_Ellipse
  - >> Square_End_XY
  - >> Square_Start_XY
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  - >> Line_End_XY
  - >> Line_Start_XY
  - >> Start_Triangle_Fill
  - >> Start_Triangle
  - >> Start_Line
  - >> Memory_24bpp_Mode
  - >> Memory_16bpp_Mode
  - >> Memory_8bpp_Mode
  - >> Memory_Linear_Mode
  - >> Memory_XY_Mode
  - >> Select_Read_Data_Position
  - >> Select_Write_Data_Position
  - >> Text_Cursor_H_V
  - >> Blinking_Time_Frames
  - >> Disable_Text_Cursor_Blinking
  - >> Enable_Text_Cursor_Blinking
  - >> Disable_Text_Cursor
  - >> Enable_Text_Cursor
  - >> Select_Graphic_Cursor_4
  - >> Select_Graphic_Cursor_3
  - >> Select_Graphic_Cursor_2
  - >> Select_Graphic_Cursor_1
  - >> Disable_Graphic_Cursor
  - >> Enable_Graphic_Cursor

  LCD_DataWrite (Thumb, 12 bytes, Stack size 4 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_DataWrite
  [Calls]
  - >> FMSC_16_DataWrite
  [Called By]
  - >> LCD_VSYNC_Pulse_Width
  - >> LCD_VSYNC_Start_Position
  - >> LCD_Vertical_Non_Display
  - >> LCD_HSYNC_Pulse_Width
  - >> LCD_HSYNC_Start_Position
  - >> LCD_Horizontal_Non_Display
  - >> LCD_HorizontalWidth_VerticalHeight
  - >> Idle_VSYNC_High
  - >> Idle_VSYNC_Low
  - >> Idle_HSYNC_High
  - >> Idle_HSYNC_Low
  - >> Idle_PDAT_High
  - >> Idle_PDAT_Low
  - >> Idle_PCLK_High
  - >> Idle_PCLK_Low
  - >> Idle_DE_High
  - >> Idle_DE_Low
  - >> DE_High_Active
  - >> DE_Low_Active
  - >> VSYNC_High_Active
  - >> VSYNC_Low_Active
  - >> HSYNC_High_Active
  - >> HSYNC_Low_Active
  - >> PDATA_IDLE_STATE
  - >> PDATA_Set_BGR
  - >> PDATA_Set_BRG
  - >> PDATA_Set_GBR
  - >> PDATA_Set_GRB
  - >> PDATA_Set_RBG
  - >> PDATA_Set_RGB
  - >> VSCAN_B_to_T
  - >> VSCAN_T_to_B
  - >> HSCAN_R_to_L
  - >> HSCAN_L_to_R
  - >> Color_Bar_OFF
  - >> Color_Bar_ON
  - >> Display_OFF
  - >> PCLK_Falling
  - >> PCLK_Rising
  - >> Select_PIP1_Window_24bpp
  - >> Select_PIP1_Window_16bpp
  - >> Select_PIP1_Window_8bpp
  - >> Select_PIP2_Window_24bpp
  - >> Select_PIP2_Window_16bpp
  - >> Select_PIP2_Window_8bpp
  - >> Select_Main_Window_24bpp
  - >> Select_Main_Window_8bpp
  - >> Select_PIP2_Parameter
  - >> Select_PIP1_Parameter
  - >> Disable_PIP2
  - >> Enable_PIP2
  - >> Disable_PIP1
  - >> Enable_PIP1
  - >> XPDAT0_Set_KIN1
  - >> XPDAT0_Set_GPIO_D0
  - >> XPDAT1_Set_KIN2
  - >> XPDAT1_Set_GPIO_D1
  - >> XPDAT2_Set_KIN4
  - >> XPDAT2_Set_GPIO_D6
  - >> XPDAT8_Set_KIN3
  - >> XPDAT8_Set_GPIO_D2
  - >> XPDAT9_Set_KOUT3
  - >> XPDAT9_Set_GPIO_D3
  - >> XPDAT16_Set_KOUT1
  - >> XPDAT16_Set_GPIO_D4
  - >> XPDAT17_Set_KOUT2
  - >> XPDAT17_Set_GPIO_D5
  - >> XPDAT18_Set_KOUT4
  - >> XPDAT18_Set_GPIO_D7
  - >> Disable_XDB7_0_PullUp
  - >> Disable_XDB15_8_PullUp
  - >> Disable_GPIOC_PullUp
  - >> Disable_GPIOD_PullUp
  - >> Disable_GPIOE_PullUp
  - >> Disable_GPIOF_PullUp
  - >> Enable_XDB7_0_PullUp
  - >> Enable_XDB15_8_PullUp
  - >> Enable_GPIOC_PullUp
  - >> Enable_GPIOD_PullUp
  - >> Enable_GPIOE_PullUp
  - >> Enable_GPIOF_PullUp
  - >> Enable_PWM0_Interrupt_Flag
  - >> Enable_PWM1_Interrupt_Flag
  - >> Enable_Draw_BTE_Interrupt_Flag
  - >> Enable_KeyScan_Interrupt_Flag
  - >> Enable_Vsync_Interrupt_Flag
  - >> Enable_I2CM_Interrupt_Flag
  - >> Enable_ExtInterrupt_Inpur_Flag
  - >> Enable_Resume_Interrupt_Flag
  - >> Mask_PWM0_Interrupt_Flag
  - >> Mask_PWM1_Interrupt_Flag
  - >> Mask_Draw_BTE_Interrupt_Flag
  - >> Mask_KeyScan_Interrupt_Flag
  - >> Mask_Vsync_Interrupt_Flag
  - >> Mask_I2CM_Interrupt_Flag
  - >> Mask_ExtInterrupt_Input_Flag
  - >> Mask_Resume_Interrupt_Flag
  - >> Clear_PWM0_Interrupt_Flag
  - >> Clear_PWM1_Interrupt_Flag
  - >> Clear_Draw_BTE_Interrupt_Flag
  - >> Clear_KeyScan_Interrupt_Flag
  - >> Clear_Vsync_Interrupt_Flag
  - >> Clear_I2CM_Interrupt_Flag
  - >> Clear_ExtInterrupt_Input_Flag
  - >> Clear_Resume_Interrupt_Flag
  - >> Disable_PWM0_Interrupt
  - >> Enable_PWM0_Interrupt
  - >> Disable_PWM1_Interrupt
  - >> Enable_PWM1_Interrupt
  - >> Disable_DMA_Draw_BTE_Interrupt
  - >> Enable_DMA_Draw_BTE_Interrupt
  - >> Disable_KeyScan_Interrupt
  - >> Enable_KeyScan_Interrupt
  - >> Disable_Vsync_Interrupt
  - >> Enable_Vsync_Interrupt
  - >> Disable_I2CM_Interrupt
  - >> Enable_I2CM_Interrupt
  - >> Disable_ExtInterrupt_Input
  - >> Enable_ExtInterrupt_Input
  - >> Disable_Resume_Interrupt
  - >> Enable_Resume_Interrupt
  - >> Memory_Select_Color_Palette_RAM
  - >> Memory_Select_Graphic_Cursor_RAM
  - >> Memory_Select_SDRAM
  - >> Text_Mode
  - >> Graphic_Mode
  - >> LVDS_Format2
  - >> LVDS_Format1
  - >> ExtInterrupt_Input_Rising_Edge_Trigger
  - >> ExtInterrupt_Input_Falling_Edge_Trigger
  - >> ExtInterrupt_Input_High_Level_Trigger
  - >> ExtInterrupt_Input_Low_Level_Trigger
  - >> ExtInterrupt_Nodebounce
  - >> ExtInterrupt_Debounce
  - >> Interrupt_Active_High
  - >> Interrupt_Active_Low
  - >> MemWrite_Down_Top_Left_Right
  - >> MemWrite_Top_Down_Left_Right
  - >> MemWrite_Right_Left_Top_Down
  - >> MemWrite_Left_Right_Top_Down
  - >> MemRead_Down_Top_Left_Right
  - >> MemRead_Top_Down_Left_Right
  - >> MemRead_Right_Left_Top_Down
  - >> MemRead_Left_Right_Top_Down
  - >> RGB_16b_24bpp_mode2
  - >> RGB_16b_24bpp_mode1
  - >> RGB_16b_16bpp
  - >> RGB_16b_8bpp
  - >> RGB_8b_24bpp
  - >> RGB_8b_16bpp
  - >> RGB_8b_8bpp
  - >> Host_Bus_16bit
  - >> Host_Bus_8bit
  - >> LT738_I2CM_Disable
  - >> LT738_I2CM_Enable
  - >> TFT_LVDS
  - >> TFT_16bit
  - >> TFT_18bit
  - >> TFT_24bit
  - >> Key_Scan_Disable
  - >> Key_Scan_Enable
  - >> LT738_WakeUp
  - >> LT738_Sleep
  - >> Enable_PLL
  - >> LT738_SW_Reset
  - >> LCD_RegisterWrite
  - >> Select_Main_Window_16bpp
  - >> Display_ON
  - >> LT738_Graphic_cursor_Init
  - >> LT738_Print_Outside_Font_String
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> LT738_PLL_Initial
  - >> System_Check_Temp
  - >> Show_picture
  - >> Show_String
  - >> Long_Key_Timing_Adjustment
  - >> Key_Scan_Wakeup_Function_Enable
  - >> Key_Scan_Freg
  - >> Long_Key_enable
  - >> Write_GPIO_F_7_0
  - >> Set_GPIO_F_In_Out
  - >> Write_GPIO_E_7_0
  - >> Set_GPIO_E_In_Out
  - >> Write_GPIO_D_7_0
  - >> Set_GPIO_D_In_Out
  - >> Write_GPIO_C_7_0
  - >> Set_GPIO_C_In_Out
  - >> Write_GPIO_B_7_4
  - >> Write_GPIO_A_7_0
  - >> Set_GPIO_A_In_Out
  - >> LT738_I2CM_Write
  - >> LT738_I2CM_Write_With_Start
  - >> LT738_I2CM_Read_With_Nack
  - >> LT738_I2CM_Read_With_Ack
  - >> LT738_I2CM_Stop
  - >> LT738_I2CM_Transmit_Data
  - >> LT738_I2CM_Clock_Prescale
  - >> Power_Saving_Sleep_Mode
  - >> Power_Saving_Suspend_Mode
  - >> Power_Saving_Standby_Mode
  - >> Power_Normal_Mode
  - >> CGRAM_Start_address
  - >> Background_color_16M
  - >> Background_color_65k
  - >> Background_color_256
  - >> Background_RGB
  - >> Foreground_color_16M
  - >> Foreground_color_65k
  - >> Foreground_color_256
  - >> Foreground_RGB
  - >> Set_Font_to_Font_Width
  - >> Font_Line_Distance
  - >> Set_GTFont_Decoder
  - >> GTFont_Select_GT22L16A1Y
  - >> GTFont_Select_GT21L24S1W
  - >> GTFont_Select_GT20L24F6Y
  - >> GTFont_Select_GT23L32S4W_GT23H32S4W
  - >> GTFont_Select_GT23L24M1Z
  - >> GTFont_Select_GT23L24T3Y_GT23H24T3Y
  - >> GTFont_Select_GT23L16U2W
  - >> GTFont_Select_GT21L16TW_GT21H16T1W
  - >> Font_Height_X4
  - >> Font_Height_X3
  - >> Font_Height_X2
  - >> Font_Height_X1
  - >> Font_Width_X4
  - >> Font_Width_X3
  - >> Font_Width_X2
  - >> Font_Width_X1
  - >> Font_90_degree
  - >> Font_0_degree
  - >> Font_Background_select_Color
  - >> Font_Background_select_Transparency
  - >> Disable_Font_Alignment
  - >> Enable_Font_Alignment
  - >> Internal_CGROM_Select_ISOIEC8859_4
  - >> Internal_CGROM_Select_ISOIEC8859_3
  - >> Internal_CGROM_Select_ISOIEC8859_2
  - >> Internal_CGROM_Select_ISOIEC8859_1
  - >> Font_Select_16x32_32x32
  - >> Font_Select_12x24_24x24
  - >> Font_Select_8x16_16x16
  - >> CGROM_Select_Genitop_FontROM
  - >> CGROM_Select_Internal_CGROM
  - >> Font_Select_UserDefine_Mode
  - >> BTE_Alpha_Blending_Effect
  - >> S1_Constant_color_16M
  - >> S1_Constant_color_65k
  - >> S1_Constant_color_256
  - >> BTE_Destination_Color_24bpp
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Destination_Color_8bpp
  - >> BTE_S1_Color_16bit_Alpha
  - >> BTE_S1_Color_8bit_Alpha
  - >> BTE_S1_Color_Constant
  - >> BTE_S1_Color_24bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S1_Color_8bpp
  - >> BTE_S0_Color_24bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_S0_Color_8bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Pattern_Format_16X16
  - >> Pattern_Format_8X8
  - >> BTE_Disable
  - >> BTE_Enable
  - >> Set_Timer1_Count_Buffer
  - >> Set_Timer1_Compare_Buffer
  - >> Set_Timer0_Count_Buffer
  - >> Set_Timer0_Compare_Buffer
  - >> Set_Timer0_Dead_Zone_Length
  - >> Stop_PWM0
  - >> Start_PWM0
  - >> One_Shot_PWM0
  - >> Auto_Reload_PWM0
  - >> Disable_PWM0_Inverter
  - >> Enable_PWM0_Inverter
  - >> Disable_PWM0_Dead_Zone
  - >> Enable_PWM0_Dead_Zone
  - >> Stop_PWM1
  - >> Start_PWM1
  - >> One_Shot_PWM1
  - >> Auto_Reload_PWM1
  - >> Disable_PWM1_Inverter
  - >> Enable_PWM1_Inverter
  - >> Select_PWM0_is_Core_Clock
  - >> Select_PWM0
  - >> Select_PWM0_is_GPIO_C7
  - >> Select_PWM1_is_Osc_Clock
  - >> Select_PWM1
  - >> Select_PWM1_is_ErrorFlag
  - >> Select_PWM0_Clock_Divided_By_8
  - >> Select_PWM0_Clock_Divided_By_4
  - >> Select_PWM0_Clock_Divided_By_2
  - >> Select_PWM0_Clock_Divided_By_1
  - >> Select_PWM1_Clock_Divided_By_8
  - >> Select_PWM1_Clock_Divided_By_4
  - >> Select_PWM1_Clock_Divided_By_2
  - >> Select_PWM1_Clock_Divided_By_1
  - >> Set_PWM_Prescaler_1_to_256
  - >> Circle_Square_Radius_RxRy
  - >> Ellipse_Radius_RxRy
  - >> Circle_Radius_R
  - >> Ellipse_Center_XY
  - >> Circle_Center_XY
  - >> Start_Circle_Square_Fill
  - >> Start_Circle_Square
  - >> Start_Square_Fill
  - >> Start_Square
  - >> Start_Right_Down_Curve_Fill
  - >> Start_Right_Up_Curve_Fill
  - >> Start_Left_Up_Curve_Fill
  - >> Start_Left_Down_Curve_Fill
  - >> Start_Right_Down_Curve
  - >> Start_Right_Up_Curve
  - >> Start_Left_Up_Curve
  - >> Start_Left_Down_Curve
  - >> Start_Circle_or_Ellipse_Fill
  - >> Start_Circle_or_Ellipse
  - >> Square_End_XY
  - >> Square_Start_XY
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  - >> Line_End_XY
  - >> Line_Start_XY
  - >> Start_Triangle_Fill
  - >> Start_Triangle
  - >> Start_Line
  - >> Memory_24bpp_Mode
  - >> Memory_16bpp_Mode
  - >> Memory_8bpp_Mode
  - >> Memory_Linear_Mode
  - >> Memory_XY_Mode
  - >> Select_Read_Data_Position
  - >> Select_Write_Data_Position
  - >> Text_Cursor_H_V
  - >> Blinking_Time_Frames
  - >> Disable_Text_Cursor_Blinking
  - >> Enable_Text_Cursor_Blinking
  - >> Disable_Text_Cursor
  - >> Enable_Text_Cursor
  - >> Select_Graphic_Cursor_4
  - >> Select_Graphic_Cursor_3
  - >> Select_Graphic_Cursor_2
  - >> Select_Graphic_Cursor_1
  - >> Disable_Graphic_Cursor
  - >> Enable_Graphic_Cursor

  LCD_DataWrite_Pixel (Thumb, 12 bytes, Stack size 4 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_DataWrite_Pixel
  [Calls]
  - >> FMSC_16_DataWrite_Pixel
  [Called By]
  - >> Display_picture
  - >> MPU_Memory_Write_Pixel_8bit
  - >> MPU_Memory_Write_Window_8bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit

  LCD_StatusRead (Thumb, 14 bytes, Stack size 4 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_StatusRead
  [Calls]
  - >> FMSC_16_StatusRead
  [Called By]
  - >> Check_Busy_Draw
  - >> Check_Interrupt_Occur
  - >> Check_NO_Interrupt
  - >> Check_Power_is_Saving
  - >> Check_Power_is_Normal
  - >> Power_Saving_Status
  - >> Check_SDRAM_Ready
  - >> Check_2D_Busy
  - >> Check_Mem_RD_FIFO_not_Empty
  - >> Check_Mem_RD_FIFO_not_Full
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> test_FSMCIO
  - >> LT738_Init
  - >> System_Check_Temp
  - >> Check_BTE_Busy

  LCD_DataRead (Thumb, 10 bytes, Stack size 0 bytes, if_port.o(.text))
  [Called By]

  - >> Idle_VSYNC_High
  - >> Idle_VSYNC_Low
  - >> Idle_HSYNC_High
  - >> Idle_HSYNC_Low
  - >> Idle_PDAT_High
  - >> Idle_PDAT_Low
  - >> Idle_PCLK_High
  - >> Idle_PCLK_Low
  - >> Idle_DE_High
  - >> Idle_DE_Low
  - >> DE_High_Active
  - >> DE_Low_Active
  - >> VSYNC_High_Active
  - >> VSYNC_Low_Active
  - >> HSYNC_High_Active
  - >> HSYNC_Low_Active
  - >> PDATA_IDLE_STATE
  - >> PDATA_Set_BGR
  - >> PDATA_Set_BRG
  - >> PDATA_Set_GBR
  - >> PDATA_Set_GRB
  - >> PDATA_Set_RBG
  - >> PDATA_Set_RGB
  - >> VSCAN_B_to_T
  - >> VSCAN_T_to_B
  - >> HSCAN_R_to_L
  - >> HSCAN_L_to_R
  - >> Color_Bar_OFF
  - >> Color_Bar_ON
  - >> Display_OFF
  - >> PCLK_Falling
  - >> PCLK_Rising
  - >> Select_PIP1_Window_24bpp
  - >> Select_PIP1_Window_16bpp
  - >> Select_PIP1_Window_8bpp
  - >> Select_PIP2_Window_24bpp
  - >> Select_PIP2_Window_16bpp
  - >> Select_PIP2_Window_8bpp
  - >> Select_Main_Window_24bpp
  - >> Select_Main_Window_8bpp
  - >> Select_PIP2_Parameter
  - >> Select_PIP1_Parameter
  - >> Disable_PIP2
  - >> Enable_PIP2
  - >> Disable_PIP1
  - >> Enable_PIP1
  - >> XPDAT0_Set_KIN1
  - >> XPDAT0_Set_GPIO_D0
  - >> XPDAT1_Set_KIN2
  - >> XPDAT1_Set_GPIO_D1
  - >> XPDAT2_Set_KIN4
  - >> XPDAT2_Set_GPIO_D6
  - >> XPDAT8_Set_KIN3
  - >> XPDAT8_Set_GPIO_D2
  - >> XPDAT9_Set_KOUT3
  - >> XPDAT9_Set_GPIO_D3
  - >> XPDAT16_Set_KOUT1
  - >> XPDAT16_Set_GPIO_D4
  - >> XPDAT17_Set_KOUT2
  - >> XPDAT17_Set_GPIO_D5
  - >> XPDAT18_Set_KOUT4
  - >> XPDAT18_Set_GPIO_D7
  - >> Disable_XDB7_0_PullUp
  - >> Disable_XDB15_8_PullUp
  - >> Disable_GPIOC_PullUp
  - >> Disable_GPIOD_PullUp
  - >> Disable_GPIOE_PullUp
  - >> Disable_GPIOF_PullUp
  - >> Enable_XDB7_0_PullUp
  - >> Enable_XDB15_8_PullUp
  - >> Enable_GPIOC_PullUp
  - >> Enable_GPIOD_PullUp
  - >> Enable_GPIOE_PullUp
  - >> Enable_GPIOF_PullUp
  - >> Enable_PWM0_Interrupt_Flag
  - >> Enable_PWM1_Interrupt_Flag
  - >> Enable_Draw_BTE_Interrupt_Flag
  - >> Enable_KeyScan_Interrupt_Flag
  - >> Enable_Vsync_Interrupt_Flag
  - >> Enable_I2CM_Interrupt_Flag
  - >> Enable_ExtInterrupt_Inpur_Flag
  - >> Enable_Resume_Interrupt_Flag
  - >> Mask_PWM0_Interrupt_Flag
  - >> Mask_PWM1_Interrupt_Flag
  - >> Mask_Draw_BTE_Interrupt_Flag
  - >> Mask_KeyScan_Interrupt_Flag
  - >> Mask_Vsync_Interrupt_Flag
  - >> Mask_I2CM_Interrupt_Flag
  - >> Mask_ExtInterrupt_Input_Flag
  - >> Mask_Resume_Interrupt_Flag
  - >> Clear_PWM0_Interrupt_Flag
  - >> Clear_PWM1_Interrupt_Flag
  - >> Clear_Draw_BTE_Interrupt_Flag
  - >> Clear_KeyScan_Interrupt_Flag
  - >> Clear_Vsync_Interrupt_Flag
  - >> Clear_I2CM_Interrupt_Flag
  - >> Clear_ExtInterrupt_Input_Flag
  - >> Clear_Resume_Interrupt_Flag
  - >> Read_Interrupt_status
  - >> Disable_PWM0_Interrupt
  - >> Enable_PWM0_Interrupt
  - >> Disable_PWM1_Interrupt
  - >> Enable_PWM1_Interrupt
  - >> Disable_DMA_Draw_BTE_Interrupt
  - >> Enable_DMA_Draw_BTE_Interrupt
  - >> Disable_KeyScan_Interrupt
  - >> Enable_KeyScan_Interrupt
  - >> Disable_Vsync_Interrupt
  - >> Enable_Vsync_Interrupt
  - >> Disable_I2CM_Interrupt
  - >> Enable_I2CM_Interrupt
  - >> Disable_ExtInterrupt_Input
  - >> Enable_ExtInterrupt_Input
  - >> Disable_Resume_Interrupt
  - >> Enable_Resume_Interrupt
  - >> Memory_Select_Color_Palette_RAM
  - >> Memory_Select_Graphic_Cursor_RAM
  - >> Memory_Select_SDRAM
  - >> Text_Mode
  - >> Graphic_Mode
  - >> LVDS_Format2
  - >> LVDS_Format1
  - >> ExtInterrupt_Input_Rising_Edge_Trigger
  - >> ExtInterrupt_Input_Falling_Edge_Trigger
  - >> ExtInterrupt_Input_High_Level_Trigger
  - >> ExtInterrupt_Input_Low_Level_Trigger
  - >> ExtInterrupt_Nodebounce
  - >> ExtInterrupt_Debounce
  - >> Interrupt_Active_High
  - >> Interrupt_Active_Low
  - >> MemWrite_Down_Top_Left_Right
  - >> MemWrite_Top_Down_Left_Right
  - >> MemWrite_Right_Left_Top_Down
  - >> MemWrite_Left_Right_Top_Down
  - >> MemRead_Down_Top_Left_Right
  - >> MemRead_Top_Down_Left_Right
  - >> MemRead_Right_Left_Top_Down
  - >> MemRead_Left_Right_Top_Down
  - >> RGB_16b_24bpp_mode2
  - >> RGB_16b_24bpp_mode1
  - >> RGB_16b_16bpp
  - >> RGB_16b_8bpp
  - >> RGB_8b_24bpp
  - >> RGB_8b_16bpp
  - >> RGB_8b_8bpp
  - >> Host_Bus_16bit
  - >> Host_Bus_8bit
  - >> LT738_I2CM_Disable
  - >> LT738_I2CM_Enable
  - >> TFT_LVDS
  - >> TFT_16bit
  - >> TFT_18bit
  - >> TFT_24bit
  - >> Key_Scan_Disable
  - >> Key_Scan_Enable
  - >> LT738_WakeUp
  - >> LT738_Sleep
  - >> Enable_PLL
  - >> LT738_SW_Reset
  - >> LCD_RegisterRead
  - >> test_FSMCIO
  - >> Select_Main_Window_16bpp
  - >> Display_ON
  - >> System_Check_Temp
  - >> Read_Key_Strobe_Data_2
  - >> Read_Key_Strobe_Data_1
  - >> Read_Key_Strobe_Data_0
  - >> Numbers_of_Key_Hit
  - >> Long_Key_Timing_Adjustment
  - >> Key_Scan_Wakeup_Function_Enable
  - >> Key_Scan_Freg
  - >> Long_Key_enable
  - >> Read_GPIO_F_7_0
  - >> Read_GPIO_E_7_0
  - >> Read_GPIO_D_7_0
  - >> Read_GPIO_C_7_0
  - >> Read_GPIO_B_7_0
  - >> Read_GPIO_A_7_0
  - >> LT738_I2CM_Arbitration
  - >> LT738_I2CM_transmit_Progress
  - >> LT738_I2CM_Bus_Busy
  - >> LT738_I2CM_Check_Slave_ACK
  - >> LT738_I2CM_Receiver_Data
  - >> GTFont_Select_GT22L16A1Y
  - >> GTFont_Select_GT21L24S1W
  - >> GTFont_Select_GT20L24F6Y
  - >> GTFont_Select_GT23L32S4W_GT23H32S4W
  - >> GTFont_Select_GT23L24M1Z
  - >> GTFont_Select_GT23L24T3Y_GT23H24T3Y
  - >> GTFont_Select_GT23L16U2W
  - >> GTFont_Select_GT21L16TW_GT21H16T1W
  - >> Font_Height_X4
  - >> Font_Height_X3
  - >> Font_Height_X2
  - >> Font_Height_X1
  - >> Font_Width_X4
  - >> Font_Width_X3
  - >> Font_Width_X2
  - >> Font_Width_X1
  - >> Font_90_degree
  - >> Font_0_degree
  - >> Font_Background_select_Color
  - >> Font_Background_select_Transparency
  - >> Disable_Font_Alignment
  - >> Enable_Font_Alignment
  - >> Internal_CGROM_Select_ISOIEC8859_4
  - >> Internal_CGROM_Select_ISOIEC8859_3
  - >> Internal_CGROM_Select_ISOIEC8859_2
  - >> Internal_CGROM_Select_ISOIEC8859_1
  - >> Font_Select_16x32_32x32
  - >> Font_Select_12x24_24x24
  - >> Font_Select_8x16_16x16
  - >> CGROM_Select_Genitop_FontROM
  - >> CGROM_Select_Internal_CGROM
  - >> Font_Select_UserDefine_Mode
  - >> BTE_Destination_Color_24bpp
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Destination_Color_8bpp
  - >> BTE_S1_Color_16bit_Alpha
  - >> BTE_S1_Color_8bit_Alpha
  - >> BTE_S1_Color_Constant
  - >> BTE_S1_Color_24bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S1_Color_8bpp
  - >> BTE_S0_Color_24bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_S0_Color_8bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Pattern_Format_16X16
  - >> Pattern_Format_8X8
  - >> BTE_Disable
  - >> BTE_Enable
  - >> Stop_PWM0
  - >> Start_PWM0
  - >> One_Shot_PWM0
  - >> Auto_Reload_PWM0
  - >> Disable_PWM0_Inverter
  - >> Enable_PWM0_Inverter
  - >> Disable_PWM0_Dead_Zone
  - >> Enable_PWM0_Dead_Zone
  - >> Stop_PWM1
  - >> Start_PWM1
  - >> One_Shot_PWM1
  - >> Auto_Reload_PWM1
  - >> Disable_PWM1_Inverter
  - >> Enable_PWM1_Inverter
  - >> Select_PWM0_is_Core_Clock
  - >> Select_PWM0
  - >> Select_PWM0_is_GPIO_C7
  - >> Select_PWM1_is_Osc_Clock
  - >> Select_PWM1
  - >> Select_PWM1_is_ErrorFlag
  - >> Select_PWM0_Clock_Divided_By_8
  - >> Select_PWM0_Clock_Divided_By_4
  - >> Select_PWM0_Clock_Divided_By_2
  - >> Select_PWM0_Clock_Divided_By_1
  - >> Select_PWM1_Clock_Divided_By_8
  - >> Select_PWM1_Clock_Divided_By_4
  - >> Select_PWM1_Clock_Divided_By_2
  - >> Select_PWM1_Clock_Divided_By_1
  - >> Memory_24bpp_Mode
  - >> Memory_16bpp_Mode
  - >> Memory_8bpp_Mode
  - >> Memory_Linear_Mode
  - >> Memory_XY_Mode
  - >> Select_Read_Data_Position
  - >> Select_Write_Data_Position
  - >> Disable_Text_Cursor_Blinking
  - >> Enable_Text_Cursor_Blinking
  - >> Disable_Text_Cursor
  - >> Enable_Text_Cursor
  - >> Select_Graphic_Cursor_4
  - >> Select_Graphic_Cursor_3
  - >> Select_Graphic_Cursor_2
  - >> Select_Graphic_Cursor_1
  - >> Disable_Graphic_Cursor
  - >> Enable_Graphic_Cursor

  Parallel_Init (Thumb, 8 bytes, Stack size 8 bytes, if_port.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = Parallel_Init ⇒ FSMC_IO_Init ⇒ GPIO_PinAFConfig
  [Calls]
  - >> FSMC_IO_Init
  [Called By]
  - >> main

  test_FSMCIO (Thumb, 38 bytes, Stack size 16 bytes, if_port.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_StatusRead
  - >> LCD_CmdWrite
  - >> __2printf

  IIC_Init (Thumb, 62 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> AT24CXX_Init

  IIC_Start (Thumb, 68 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Stop (Thumb, 62 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte
  - >> IIC_Wait_Ack

  IIC_Wait_Ack (Thumb, 82 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop
  [Calls]
  - >> delay_us
  - >> IIC_Stop
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Ack (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Ack
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_NAck (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_NAck
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_Send_Byte (Thumb, 90 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Read_Byte (Thumb, 94 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> delay_us
  - >> IIC_NAck
  - >> IIC_Ack
  [Called By]
  - >> AT24CXX_ReadOneByte

  AT24CXX_Init (Thumb, 8 bytes, Stack size 8 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = AT24CXX_Init ⇒ IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Init
  [Called By]
  - >> TP_Init

  AT24CXX_ReadOneByte (Thumb, 88 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> TP_Get_Adjdata
  - >> AT24CXX_Read
  - >> AT24CXX_Check
  - >> AT24CXX_ReadLenByte

  AT24CXX_WriteOneByte (Thumb, 80 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> delay_ms
  [Called By]
  - >> TP_Save_Adjdata
  - >> AT24CXX_Write
  - >> AT24CXX_Check
  - >> AT24CXX_WriteLenByte

  AT24CXX_WriteLenByte (Thumb, 42 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Save_Adjdata

  AT24CXX_ReadLenByte (Thumb, 44 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Get_Adjdata

  AT24CXX_Check (Thumb, 46 bytes, Stack size 8 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  AT24CXX_Read (Thumb, 34 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_ReadOneByte

  AT24CXX_Write (Thumb, 36 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte

  CT_Delay (Thumb, 10 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CT_Delay
  [Calls]
  - >> delay_us
  [Called By]
  - >> CT_IIC_Read_Byte
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start

  CT_IIC_Init (Thumb, 60 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = CT_IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> GT9147_Init

  CT_IIC_Start (Thumb, 62 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Start ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  - >> delay_us
  [Called By]
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg

  CT_IIC_Stop (Thumb, 56 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Stop ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  - >> delay_us
  [Called By]
  - >> CT_IIC_Wait_Ack
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg

  CT_IIC_Wait_Ack (Thumb, 78 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CT_IIC_Wait_Ack ⇒ CT_IIC_Stop ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Stop
  - >> CT_Delay
  [Called By]
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg

  CT_IIC_Ack (Thumb, 66 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Ack ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_NAck (Thumb, 66 bytes, Stack size 8 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_Send_Byte (Thumb, 82 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CT_IIC_Send_Byte ⇒ CT_Delay
  [Calls]
  - >> CT_Delay
  [Called By]
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg

  CT_IIC_Read_Byte (Thumb, 92 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CT_IIC_Read_Byte ⇒ CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> CT_Delay
  - >> delay_us
  [Called By]
  - >> GT9147_RD_Reg

  TP_Write_Byte (Thumb, 64 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TP_Write_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> TP_Read_AD

  TP_Read_AD (Thumb, 132 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 120 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 38 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Init
  - >> TP_Read_XY2

  TP_Read_XY2 (Thumb, 192 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 72 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = TP_Drow_Touch_Point ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LT738_DrawLine
  - >> LT738_DrawCircle
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 22 bytes, Stack size 16 bytes, touch.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawCircle_Fill

  LCD_ShowChar (Thumb, 278 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = LCD_ShowChar ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LT738_DrawLine
  [Called By]
  - >> LCD_ShowNum

  LCD_Pow (Thumb, 22 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Pow
  [Called By]
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 188 bytes, Stack size 56 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show

  TP_Scan (Thumb, 242 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XY2
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 128 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = TP_Save_Adjdata ⇒ AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteLenByte
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Get_Adjdata (Thumb, 170 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = TP_Get_Adjdata ⇒ AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadLenByte
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 348 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 188
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_ShowNum
  - >> LT738_Print_Internal_Font_String
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 1896 bytes, Stack size 96 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Drow_Touch_Point
  - >> delay_ms
  - >> LT738_Print_Internal_Font_String
  - >> LT738_DrawSquare_Fill
  - >> __hardfp_sqrt
  - >> __aeabi_f2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_dmul
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  [Called By]
  - >> TP_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 162 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 300
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> TP_Adjust
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Read_XY
  - >> AT24CXX_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> LT738_DrawSquare_Fill
  [Address Reference Count : 1]
  - touch.o(.data)

  LCD_RegisterWrite (Thumb, 20 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> PIP_Window_Image_Start_XY
  - >> PIP_Image_Width
  - >> PIP_Image_Start_Address
  - >> PIP_Display_Start_XY
  - >> Main_Window_Start_XY
  - >> Main_Image_Width
  - >> Main_Image_Start_Address
  - >> Canvas_image_width
  - >> Canvas_Image_Start_address
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> LT738_SDRAM_initail
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S1_Window_Start_XY
  - >> BTE_S1_Image_Width
  - >> BTE_S1_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> Goto_Text_XY
  - >> Goto_Linear_Addr
  - >> Goto_Pixel_XY
  - >> Set_Graphic_Cursor_Color_2
  - >> Set_Graphic_Cursor_Color_1
  - >> Graphic_Cursor_XY
  - >> PIP_Window_Width_Height

  LCD_RegisterRead (Thumb, 20 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Check_Mem_WR_FIFO_not_Full (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Check_Mem_WR_FIFO_not_Full ⇒ LCD_StatusRead
  [Calls]
  - >> LCD_StatusRead
  [Called By]
  - >> Display_picture
  - >> MPU_Memory_Write_Window_8bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_Print_Outside_Font_String
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> Show_picture
  - >> Show_String

  Check_Mem_WR_FIFO_Empty (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Check_Mem_WR_FIFO_Empty ⇒ LCD_StatusRead
  [Calls]
  - >> LCD_StatusRead
  [Called By]
  - >> Display_picture
  - >> MPU_Memory_Write_Pixel_8bit
  - >> MPU_Memory_Write_Window_8bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write

  Check_Mem_RD_FIFO_not_Full (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead

  Check_Mem_RD_FIFO_not_Empty (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead

  Check_2D_Busy (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Check_2D_Busy ⇒ LCD_StatusRead
  [Calls]
  - >> LCD_StatusRead
  [Called By]
  - >> LT738_DrawLine
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawCircle_Fill
  - >> LT738_DrawCircle
  - >> LT738_Print_Outside_Font_String
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawRightDownCurve_Fill
  - >> LT738_DrawRightUpCurve_Fill
  - >> LT738_DrawLeftDownCurve_Fill
  - >> LT738_DrawLeftUpCurve_Fill
  - >> LT738_DrawRightDownCurve
  - >> LT738_DrawRightUpCurve
  - >> LT738_DrawLeftDownCurve
  - >> LT738_DrawLeftUpCurve
  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle
  - >> LT738_DrawCircleSquare_Fill
  - >> LT738_DrawCircleSquare
  - >> LT738_DrawEllipse_Fill
  - >> LT738_DrawEllipse
  - >> Show_String

  Check_SDRAM_Ready (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Check_SDRAM_Ready ⇒ LCD_StatusRead
  [Calls]
  - >> LCD_StatusRead
  [Called By]
  - >> LT738_SDRAM_initail

  Power_Saving_Status (Thumb, 24 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead

  Check_Power_is_Normal (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead
  [Called By]
  - >> LT738_Wkup_Sleep
  - >> LT738_Wkup_Suspend
  - >> LT738_Wkup_Standby

  Check_Power_is_Saving (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead
  [Called By]
  - >> LT738_SleepMode
  - >> LT738_Suspend
  - >> LT738_Standby

  Check_NO_Interrupt (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead

  Check_Interrupt_Occur (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead

  Check_Busy_Draw (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> LCD_StatusRead
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> Start_Circle_Square_Fill
  - >> Start_Circle_Square
  - >> Start_Square_Fill
  - >> Start_Square
  - >> Start_Right_Down_Curve_Fill
  - >> Start_Right_Up_Curve_Fill
  - >> Start_Left_Up_Curve_Fill
  - >> Start_Left_Down_Curve_Fill
  - >> Start_Right_Down_Curve
  - >> Start_Right_Up_Curve
  - >> Start_Left_Up_Curve
  - >> Start_Left_Down_Curve
  - >> Start_Circle_or_Ellipse_Fill
  - >> Start_Circle_or_Ellipse
  - >> Start_Triangle_Fill
  - >> Start_Triangle
  - >> Start_Line

  LT738_SW_Reset (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PLL (Thumb, 32 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Delay_us

  LT738_Sleep (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_WakeUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Key_Scan_Enable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Key_Scan_Disable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  TFT_24bit (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  TFT_18bit (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  TFT_16bit (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TFT_16bit ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  TFT_LVDS (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Enable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Disable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Host_Bus_8bit (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Host_Bus_16bit (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Host_Bus_16bit ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  RGB_8b_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  RGB_8b_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  RGB_8b_24bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  RGB_16b_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  RGB_16b_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RGB_16b_16bpp ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> Set_LCD_Panel

  RGB_16b_24bpp_mode1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  RGB_16b_24bpp_mode2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemRead_Left_Right_Top_Down (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemRead_Right_Left_Top_Down (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemRead_Top_Down_Left_Right (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemRead_Down_Top_Left_Right (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemWrite_Left_Right_Top_Down (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = MemWrite_Left_Right_Top_Down ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  MemWrite_Right_Left_Top_Down (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemWrite_Top_Down_Left_Right (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  MemWrite_Down_Top_Left_Right (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Interrupt_Active_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Interrupt_Active_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Debounce (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Nodebounce (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Input_Low_Level_Trigger (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Input_High_Level_Trigger (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Input_Falling_Edge_Trigger (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  ExtInterrupt_Input_Rising_Edge_Trigger (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LVDS_Format1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LVDS_Format2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Graphic_Mode (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Graphic_Mode ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Display_picture
  - >> MPU_Memory_Write_Pixel_8bit
  - >> MPU_Memory_Write_Window_8bit
  - >> LT738_Graphic_cursor_Init
  - >> LT738_Print_Outside_Font_String
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> Set_LCD_Panel
  - >> Show_String

  Text_Mode (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Text_Mode ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Print_Internal_Font_String
  - >> LT738_Print_Outside_Font_String
  - >> Show_String

  Memory_Select_SDRAM (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Memory_Select_SDRAM ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Graphic_cursor_Init
  - >> Set_LCD_Panel

  Memory_Select_Graphic_Cursor_RAM (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Graphic_cursor_Init

  Memory_Select_Color_Palette_RAM (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Resume_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_Resume_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_ExtInterrupt_Input (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_ExtInterrupt_Input (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_I2CM_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_I2CM_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Vsync_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_Vsync_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_KeyScan_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_KeyScan_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_DMA_Draw_BTE_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_DMA_Draw_BTE_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM1_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_PWM1_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM0_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_PWM0_Interrupt (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_Interrupt_status (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Clear_Resume_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_ExtInterrupt_Input_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_I2CM_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_Vsync_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_KeyScan_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_Draw_BTE_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_PWM1_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Clear_PWM0_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_Resume_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_ExtInterrupt_Input_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_I2CM_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_Vsync_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_KeyScan_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_Draw_BTE_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_PWM1_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Mask_PWM0_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Resume_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_ExtInterrupt_Inpur_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_I2CM_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Vsync_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_KeyScan_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Draw_BTE_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM1_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM0_Interrupt_Flag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_GPIOF_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_GPIOE_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_GPIOD_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_GPIOC_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_XDB15_8_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_XDB7_0_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_GPIOF_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_GPIOE_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_GPIOD_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_GPIOC_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_XDB15_8_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_XDB7_0_PullUp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT18_Set_GPIO_D7 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT18_Set_KOUT4 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT17_Set_GPIO_D5 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT17_Set_KOUT2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT16_Set_GPIO_D4 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT16_Set_KOUT1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT9_Set_GPIO_D3 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT9_Set_KOUT3 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT8_Set_GPIO_D2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT8_Set_KIN3 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT2_Set_GPIO_D6 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT2_Set_KIN4 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT1_Set_GPIO_D1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT1_Set_KIN2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT0_Set_GPIO_D0 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  XPDAT0_Set_KIN1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PIP1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Disable_PIP1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Enable_PIP2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Disable_PIP2 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Select_PIP1_Parameter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Select_PIP2_Parameter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  Select_Main_Window_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_Main_Window_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_Main_Window_16bpp ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> main

  Select_Main_Window_24bpp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Show

  Select_PIP2_Window_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PIP2_Window_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PIP_Init

  Select_PIP2_Window_24bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PIP1_Window_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PIP1_Window_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PIP_Init

  Select_PIP1_Window_24bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PCLK_Rising (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = PCLK_Rising ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  PCLK_Falling (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Display_ON (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Display_ON ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> main

  Display_OFF (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Color_Bar_ON (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Color_Bar_ON

  Color_Bar_OFF (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Color_Bar_OFF

  HSCAN_L_to_R (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  HSCAN_R_to_L (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  VSCAN_T_to_B (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = VSCAN_T_to_B ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  VSCAN_B_to_T (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_Set_RGB (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = PDATA_Set_RGB ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  PDATA_Set_RBG (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_Set_GRB (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_Set_GBR (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_Set_BRG (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_Set_BGR (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  PDATA_IDLE_STATE (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  HSYNC_Low_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = HSYNC_Low_Active ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  HSYNC_High_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  VSYNC_Low_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  VSYNC_High_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = VSYNC_High_Active ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  DE_Low_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DE_Low_Active ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  DE_High_Active (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_DE_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_DE_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_PCLK_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_PCLK_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_PDAT_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_PDAT_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_HSYNC_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_HSYNC_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_VSYNC_Low (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Idle_VSYNC_High (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LCD_HorizontalWidth_VerticalHeight (Thumb, 160 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_HorizontalWidth_VerticalHeight ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_Horizontal_Non_Display (Thumb, 90 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_Horizontal_Non_Display ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_HSYNC_Start_Position (Thumb, 50 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_HSYNC_Start_Position ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_HSYNC_Pulse_Width (Thumb, 50 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_HSYNC_Pulse_Width ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_Vertical_Non_Display (Thumb, 34 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_Vertical_Non_Display ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_VSYNC_Start_Position (Thumb, 22 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_VSYNC_Start_Position ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  LCD_VSYNC_Pulse_Width (Thumb, 22 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_VSYNC_Pulse_Width ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  Main_Image_Start_Address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Main_Image_Start_Address ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> main
  - >> Show

  Main_Image_Width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Main_Image_Width ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> main
  - >> Show

  Main_Window_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Main_Window_Start_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> main
  - >> Show

  PIP_Display_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_Set_DisWindowPos
  - >> LT738_PIP_Init

  PIP_Image_Start_Address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_PIP_Init

  PIP_Image_Width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_PIP_Init

  PIP_Window_Image_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_PIP_Init

  PIP_Window_Width_Height (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_PIP_Init

  Enable_Graphic_Cursor (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Enable_Graphic_Cursor
  - >> LT738_Graphic_cursor_Init

  Disable_Graphic_Cursor (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Disable_Graphic_Cursor

  Select_Graphic_Cursor_1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_Graphic_cursor_Pos
  - >> LT738_Graphic_cursor_Init

  Select_Graphic_Cursor_2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_Graphic_cursor_Pos
  - >> LT738_Graphic_cursor_Init

  Select_Graphic_Cursor_3 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_Graphic_cursor_Pos
  - >> LT738_Graphic_cursor_Init

  Select_Graphic_Cursor_4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Set_Graphic_cursor_Pos
  - >> LT738_Graphic_cursor_Init

  Enable_Text_Cursor (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Enable_Text_Cursor
  - >> LT738_Text_cursor_Init

  Disable_Text_Cursor (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Disable_Text_Cursor

  Enable_Text_Cursor_Blinking (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Text_cursor_Init

  Disable_Text_Cursor_Blinking (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Text_cursor_Init

  Blinking_Time_Frames (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Text_cursor_Init

  Text_Cursor_H_V (Thumb, 32 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Text_cursor_Init

  Graphic_Cursor_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_Set_Graphic_cursor_Pos
  - >> LT738_Graphic_cursor_Init

  Set_Graphic_Cursor_Color_1 (Thumb, 14 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_Graphic_cursor_Init

  Set_Graphic_Cursor_Color_2 (Thumb, 14 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_Graphic_cursor_Init

  Canvas_Image_Start_address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Canvas_Image_Start_address ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> main
  - >> Show

  Canvas_image_width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Canvas_image_width ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> main
  - >> Show

  Active_Window_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Active_Window_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> Display_picture
  - >> main
  - >> MPU_Memory_Write_Window_8bit
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> Show

  Active_Window_WH (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Active_Window_WH ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> Display_picture
  - >> main
  - >> MPU_Memory_Write_Window_8bit
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write
  - >> Show

  Select_Write_Data_Position (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_Read_Data_Position (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Memory_XY_Mode (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Memory_XY_Mode ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  Memory_Linear_Mode (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Memory_8bpp_Mode (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Memory_16bpp_Mode (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Memory_16bpp_Mode ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> Set_LCD_Panel

  Memory_24bpp_Mode (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Goto_Pixel_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Goto_Pixel_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> Display_picture
  - >> MPU_Memory_Write_Pixel_8bit
  - >> MPU_Memory_Write_Window_8bit
  - >> MPU16_24bpp_Mode2_Memory_Write
  - >> MPU16_24bpp_Mode1_Memory_Write
  - >> MPU16_16bpp_Memory_Write
  - >> MPU8_24bpp_Memory_Write
  - >> MPU8_16bpp_Memory_Write
  - >> MPU8_8bpp_Memory_Write

  Goto_Linear_Addr (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite

  Goto_Text_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Goto_Text_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_RegisterWrite
  [Called By]
  - >> LT738_Print_Internal_Font_String
  - >> LT738_Print_Outside_Font_String

  Start_Line (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Start_Line ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLine

  Start_Triangle (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawTriangle

  Start_Triangle_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawTriangle_Fill

  Line_Start_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Line_Start_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLine

  Line_End_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLine

  Triangle_Point1_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle

  Triangle_Point2_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle

  Triangle_Point3_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle

  Square_Start_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Square_Start_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawCircleSquare_Fill
  - >> LT738_DrawCircleSquare

  Square_End_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Square_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawCircleSquare_Fill
  - >> LT738_DrawCircleSquare

  Start_Circle_or_Ellipse (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Start_Circle_or_Ellipse ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircle
  - >> LT738_DrawEllipse

  Start_Circle_or_Ellipse_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Start_Circle_or_Ellipse_Fill ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircle_Fill
  - >> LT738_DrawEllipse_Fill

  Start_Left_Down_Curve (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLeftDownCurve

  Start_Left_Up_Curve (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLeftUpCurve

  Start_Right_Up_Curve (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawRightUpCurve

  Start_Right_Down_Curve (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawRightDownCurve

  Start_Left_Down_Curve_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLeftDownCurve_Fill

  Start_Left_Up_Curve_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLeftUpCurve_Fill

  Start_Right_Up_Curve_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawRightUpCurve_Fill

  Start_Right_Down_Curve_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawRightDownCurve_Fill

  Start_Square (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Start_Square ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawSquare

  Start_Square_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Start_Square_Fill ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawSquare_Fill

  Start_Circle_Square (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircleSquare

  Start_Circle_Square_Fill (Thumb, 20 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircleSquare_Fill

  Circle_Center_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Circle_Center_XY ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircle_Fill
  - >> LT738_DrawCircle

  Ellipse_Center_XY (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawRightDownCurve_Fill
  - >> LT738_DrawRightUpCurve_Fill
  - >> LT738_DrawLeftDownCurve_Fill
  - >> LT738_DrawLeftUpCurve_Fill
  - >> LT738_DrawRightDownCurve
  - >> LT738_DrawRightUpCurve
  - >> LT738_DrawLeftDownCurve
  - >> LT738_DrawLeftUpCurve
  - >> LT738_DrawEllipse_Fill
  - >> LT738_DrawEllipse

  Circle_Radius_R (Thumb, 54 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Circle_Radius_R ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircle_Fill
  - >> LT738_DrawCircle

  Ellipse_Radius_RxRy (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawRightDownCurve_Fill
  - >> LT738_DrawRightUpCurve_Fill
  - >> LT738_DrawLeftDownCurve_Fill
  - >> LT738_DrawLeftUpCurve_Fill
  - >> LT738_DrawRightDownCurve
  - >> LT738_DrawRightUpCurve
  - >> LT738_DrawLeftDownCurve
  - >> LT738_DrawLeftUpCurve
  - >> LT738_DrawEllipse_Fill
  - >> LT738_DrawEllipse

  Circle_Square_Radius_RxRy (Thumb, 56 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawCircleSquare_Fill
  - >> LT738_DrawCircleSquare

  Set_PWM_Prescaler_1_to_256 (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Set_PWM_Prescaler_1_to_256 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init
  - >> LT738_PWM0_Init

  Select_PWM1_Clock_Divided_By_1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_PWM1_Clock_Divided_By_1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Select_PWM1_Clock_Divided_By_2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_PWM1_Clock_Divided_By_2 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Select_PWM1_Clock_Divided_By_4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_PWM1_Clock_Divided_By_4 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Select_PWM1_Clock_Divided_By_8 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_PWM1_Clock_Divided_By_8 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Select_PWM0_Clock_Divided_By_1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Select_PWM0_Clock_Divided_By_2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Select_PWM0_Clock_Divided_By_4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Select_PWM0_Clock_Divided_By_8 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Select_PWM1_is_ErrorFlag (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PWM1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Select_PWM1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Select_PWM1_is_Osc_Clock (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PWM0_is_GPIO_C7 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Select_PWM0 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Select_PWM0_is_Core_Clock (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM1_Inverter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_PWM1_Inverter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Auto_Reload_PWM1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  One_Shot_PWM1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Start_PWM1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Start_PWM1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Stop_PWM1 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Stop_PWM1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  Enable_PWM0_Dead_Zone (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_PWM0_Dead_Zone (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_PWM0_Inverter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Disable_PWM0_Inverter (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Auto_Reload_PWM0 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  One_Shot_PWM0 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Start_PWM0 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Stop_PWM0 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Set_Timer0_Dead_Zone_Length (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Set_Timer0_Compare_Buffer (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Duty
  - >> LT738_PWM0_Init

  Set_Timer0_Count_Buffer (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM0_Init

  Set_Timer1_Compare_Buffer (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Set_Timer1_Compare_Buffer ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init
  - >> LT738_PWM1_Duty

  Set_Timer1_Count_Buffer (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Set_Timer1_Count_Buffer ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_PWM1_Init

  BTE_Enable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Disable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Check_BTE_Busy (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_StatusRead
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  Pattern_Format_8X8 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill

  Pattern_Format_16X16 (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill

  BTE_ROP_Code (Thumb, 34 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Operation_Code (Thumb, 30 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_S0_Color_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_S0_Color_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy

  BTE_S0_Color_24bpp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Color_8bpp (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Color_16bpp (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Memory_Copy

  BTE_S1_Color_24bpp (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Color_Constant (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Color_8bit_Alpha (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Color_16bit_Alpha (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_Destination_Color_8bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_Destination_Color_16bpp (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Destination_Color_24bpp (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S0_Memory_Start_Address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_S0_Image_Width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_S0_Window_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_S1_Memory_Start_Address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Memory_Copy

  S1_Constant_color_256 (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  S1_Constant_color_65k (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  S1_Constant_color_16M (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  BTE_S1_Image_Width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Memory_Copy

  BTE_S1_Window_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Memory_Copy

  BTE_Destination_Memory_Start_Address (Thumb, 42 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Destination_Image_Width (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Destination_Window_Start_XY (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Window_Size (Thumb, 40 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_RegisterWrite
  [Called By]
  - >> BTE_Alpha_Blending
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Pattern_Fill
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_BTE_Memory_Copy
  - >> BTE_Solid_Fill
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  BTE_Alpha_Blending_Effect (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> BTE_Alpha_Blending

  Font_Select_UserDefine_Mode (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Print_Outside_Font_String

  CGROM_Select_Internal_CGROM (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CGROM_Select_Internal_CGROM ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Print_Internal_Font_String
  - >> LT738_Print_Outside_Font_String

  CGROM_Select_Genitop_FontROM (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Font_Select_8x16_16x16 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Select_8x16_16x16 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Select_12x24_24x24 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Select_12x24_24x24 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Select_16x32_32x32 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Select_16x32_32x32 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Internal_CGROM_Select_ISOIEC8859_1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Internal_CGROM_Select_ISOIEC8859_2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Internal_CGROM_Select_ISOIEC8859_3 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Internal_CGROM_Select_ISOIEC8859_4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Enable_Font_Alignment (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Enable_Font_Alignment ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Disable_Font_Alignment (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Disable_Font_Alignment ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Background_select_Transparency (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Background_select_Transparency ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Background_select_Color (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Background_select_Color ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_0_degree (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Font_90_degree (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Font_Width_X1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Width_X1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Width_X2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Width_X2 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Width_X3 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Width_X3 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Width_X4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Width_X4 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Height_X1 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Height_X1 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Height_X2 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Height_X2 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Height_X3 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Height_X3 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  Font_Height_X4 (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Font_Height_X4 ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Select_Internal_Font_Init

  GTFont_Select_GT21L16TW_GT21H16T1W (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT23L16U2W (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT23L24T3Y_GT23H24T3Y (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT23L24M1Z (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT23L32S4W_GT23H32S4W (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT20L24F6Y (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT21L24S1W (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  GTFont_Select_GT22L16A1Y (Thumb, 34 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Set_GTFont_Decoder (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Font_Line_Distance (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Set_Font_to_Font_Width (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Foreground_RGB (Thumb, 46 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Foreground_color_256 (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  Foreground_color_65k (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Foreground_color_65k ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_DrawLine
  - >> LT738_Print_Internal_Font_String
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawCircle_Fill
  - >> LT738_DrawCircle
  - >> LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> BTE_Solid_Fill
  - >> LT738_Print_Outside_Font_String
  - >> LT738_DrawPentagon_Fill
  - >> LT738_DrawPentagon
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral
  - >> LT738_DrawRightDownCurve_Fill
  - >> LT738_DrawRightUpCurve_Fill
  - >> LT738_DrawLeftDownCurve_Fill
  - >> LT738_DrawLeftUpCurve_Fill
  - >> LT738_DrawRightDownCurve
  - >> LT738_DrawRightUpCurve
  - >> LT738_DrawLeftDownCurve
  - >> LT738_DrawLeftUpCurve
  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle
  - >> LT738_DrawCircleSquare_Fill
  - >> LT738_DrawCircleSquare
  - >> LT738_DrawEllipse_Fill
  - >> LT738_DrawEllipse

  Foreground_color_16M (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Background_RGB (Thumb, 46 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Background_color_256 (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_BTE_Memory_Copy_ColorExpansion_8

  Background_color_65k (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Background_color_65k ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Print_Internal_Font_String
  - >> LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit
  - >> LT738_BTE_MCU_Write_Chroma_key_MCU_16bit
  - >> LT738_BTE_Pattern_Fill_With_Chroma_key
  - >> LT738_BTE_Memory_Copy_Chroma_key
  - >> LT738_Print_Outside_Font_String

  Background_color_16M (Thumb, 46 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  CGRAM_Start_address (Thumb, 58 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Power_Normal_Mode (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Wkup_Sleep
  - >> LT738_Wkup_Suspend
  - >> LT738_Wkup_Standby

  Power_Saving_Standby_Mode (Thumb, 28 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Standby

  Power_Saving_Suspend_Mode (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Suspend

  Power_Saving_Sleep_Mode (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_SleepMode

  LT738_I2CM_Clock_Prescale (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Transmit_Data (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Receiver_Data (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  LT738_I2CM_Stop (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Read_With_Ack (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Read_With_Nack (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Write_With_Start (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Write (Thumb, 16 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  LT738_I2CM_Check_Slave_ACK (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  LT738_I2CM_Bus_Busy (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  LT738_I2CM_transmit_Progress (Thumb, 30 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  LT738_I2CM_Arbitration (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Set_GPIO_A_In_Out (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Write_GPIO_A_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_A_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Write_GPIO_B_7_4 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_B_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Set_GPIO_C_In_Out (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Write_GPIO_C_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_C_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Set_GPIO_D_In_Out (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Write_GPIO_D_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_D_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Set_GPIO_E_In_Out (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Write_GPIO_E_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_E_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Set_GPIO_F_In_Out (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Write_GPIO_F_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Read_GPIO_F_7_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Long_Key_enable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Key_Scan_Freg (Thumb, 34 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Key_Scan_Wakeup_Function_Enable (Thumb, 26 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Long_Key_Timing_Adjustment (Thumb, 30 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Numbers_of_Key_Hit (Thumb, 22 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Read_Key_Strobe_Data_0 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Read_Key_Strobe_Data_1 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Read_Key_Strobe_Data_2 (Thumb, 18 bytes, Stack size 8 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> LCD_DataRead
  - >> LCD_CmdWrite

  Show_String (Thumb, 44 bytes, Stack size 8 bytes, lt738.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Show_String ⇒ Text_Mode ⇒ LCD_DataWrite
  [Calls]
  - >> Text_Mode
  - >> Graphic_Mode
  - >> Check_2D_Busy
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  [Called By]
  - >> LT738_Print_Internal_Font_String

  Show_picture (Thumb, 36 bytes, Stack size 16 bytes, lt738.o(.text), UNUSED)
  [Calls]

  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite

  Display_picture (Thumb, 152 bytes, Stack size 56 bytes, lt738_demo.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = Display_picture ⇒ Active_Window_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY
  [Called By]
  - >> main

  GRAY_32 (Thumb, 56 bytes, Stack size 16 bytes, lt738_demo.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = GRAY_32 ⇒ LT738_DrawSquare_Fill ⇒ Start_Square_Fill ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> LT738_DrawSquare_Fill
  [Called By]
  - >> main

  WB_block (Thumb, 324 bytes, Stack size 32 bytes, lt738_demo.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = WB_block ⇒ LT738_DrawSquare_Fill ⇒ Start_Square_Fill ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> LT738_DrawSquare_Fill
  [Called By]
  - >> main

  Show (Thumb, 142 bytes, Stack size 8 bytes, lt738_demo.o(.text), UNUSED)
  [Calls]

  - >> Select_Main_Window_24bpp
  - >> WaitKey
  - >> Main_Window_Start_XY
  - >> Main_Image_Width
  - >> Main_Image_Start_Address
  - >> LT738_DrawSquare_Fill
  - >> Canvas_image_width
  - >> Canvas_Image_Start_address
  - >> Active_Window_XY
  - >> Active_Window_WH

  LT738_HW_Reset (Thumb, 98 bytes, Stack size 16 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LT738_HW_Reset ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> Delay_ms
  - >> GPIO_ResetBits
  [Called By]
  - >> LT738_Init
  - >> System_Check_Temp

  System_Check_Temp (Thumb, 108 bytes, Stack size 16 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = System_Check_Temp ⇒ LT738_HW_Reset ⇒ GPIO_Init
  [Calls]
  - >> LCD_DataRead
  - >> LCD_StatusRead
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Delay_ms
  - >> LT738_HW_Reset
  [Called By]
  - >> LT738_Init

  LT738_PLL_Initial (Thumb, 278 bytes, Stack size 48 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = LT738_PLL_Initial ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Delay_us
  - >> Delay_ms
  [Called By]
  - >> LT738_initial

  LT738_SDRAM_initail (Thumb, 78 bytes, Stack size 16 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LT738_SDRAM_initail ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> Check_SDRAM_Ready
  - >> LCD_RegisterWrite
  - >> Delay_ms
  [Called By]
  - >> LT738_Wkup_Suspend
  - >> LT738_Suspend
  - >> LT738_initial

  Set_LCD_Panel (Thumb, 108 bytes, Stack size 8 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Set_LCD_Panel ⇒ LCD_VSYNC_Pulse_Width ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_VSYNC_Pulse_Width
  - >> LCD_VSYNC_Start_Position
  - >> LCD_Vertical_Non_Display
  - >> LCD_HSYNC_Pulse_Width
  - >> LCD_HSYNC_Start_Position
  - >> LCD_Horizontal_Non_Display
  - >> LCD_HorizontalWidth_VerticalHeight
  - >> DE_Low_Active
  - >> VSYNC_High_Active
  - >> HSYNC_Low_Active
  - >> PDATA_Set_RGB
  - >> VSCAN_T_to_B
  - >> PCLK_Rising
  - >> Memory_Select_SDRAM
  - >> Graphic_Mode
  - >> MemWrite_Left_Right_Top_Down
  - >> RGB_16b_16bpp
  - >> Host_Bus_16bit
  - >> TFT_16bit
  - >> Memory_16bpp_Mode
  - >> Memory_XY_Mode
  [Called By]
  - >> LT738_initial

  LT738_initial (Thumb, 20 bytes, Stack size 8 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = LT738_initial ⇒ LT738_PLL_Initial ⇒ LCD_DataWrite
  [Calls]
  - >> Set_LCD_Panel
  - >> LT738_SDRAM_initail
  - >> LT738_PLL_Initial
  [Called By]
  - >> LT738_Init

  LT738_Init (Thumb, 56 bytes, Stack size 8 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = LT738_Init ⇒ LT738_initial ⇒ LT738_PLL_Initial ⇒ LCD_DataWrite
  [Calls]
  - >> LCD_StatusRead
  - >> Delay_ms
  - >> LT738_initial
  - >> System_Check_Temp
  - >> LT738_HW_Reset
  [Called By]
  - >> main

  MPU8_8bpp_Memory_Write (Thumb, 98 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU8_16bpp_Memory_Write (Thumb, 110 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU8_24bpp_Memory_Write (Thumb, 154 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU16_16bpp_Memory_Write (Thumb, 98 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU16_24bpp_Mode1_Memory_Write (Thumb, 128 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU16_24bpp_Mode2_Memory_Write (Thumb, 110 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  LT738_DrawLine (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LT738_DrawLine ⇒ Line_End_XY ⇒ LCD_DataWrite
  [Calls]
  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Line_End_XY
  - >> Line_Start_XY
  - >> Start_Line
  [Called By]
  - >> LCD_ShowChar
  - >> TP_Drow_Touch_Point
  - >> LT738_DrawCylinder
  - >> LT738_DrawLine_Width

  LT738_DrawLine_Width (Thumb, 246 bytes, Stack size 80 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawLine
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dneg
  [Called By]
  - >> LT738_MakeTable

  LT738_DrawCircle (Thumb, 44 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LT738_DrawCircle ⇒ Circle_Center_XY ⇒ LCD_DataWrite
  [Calls]
  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Circle_Radius_R
  - >> Circle_Center_XY
  - >> Start_Circle_or_Ellipse
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> main

  LT738_DrawCircle_Fill (Thumb, 44 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LT738_DrawCircle_Fill ⇒ Circle_Center_XY ⇒ LCD_DataWrite
  [Calls]
  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Circle_Radius_R
  - >> Circle_Center_XY
  - >> Start_Circle_or_Ellipse_Fill
  [Called By]
  - >> TP_Draw_Big_Point
  - >> lcd_draw_bline
  - >> LT738_DrawCircle_Width

  LT738_DrawCircle_Width (Thumb, 48 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawCircle_Fill

  LT738_DrawEllipse (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Circle_or_Ellipse
  [Called By]
  - >> LT738_DrawCylinder

  LT738_DrawEllipse_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Circle_or_Ellipse_Fill
  [Called By]
  - >> LT738_DrawCylinder
  - >> LT738_DrawEllipse_Width

  LT738_DrawEllipse_Width (Thumb, 58 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawEllipse_Fill

  LT738_DrawSquare (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LT738_DrawSquare ⇒ Start_Square ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Start_Square
  - >> Square_End_XY
  - >> Square_Start_XY
  [Called By]
  - >> main
  - >> LT738_DrawQuadrangular

  LT738_DrawSquare_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = LT738_DrawSquare_Fill ⇒ Start_Square_Fill ⇒ Check_Busy_Draw ⇒ LCD_StatusRead
  [Calls]
  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Start_Square_Fill
  - >> Square_End_XY
  - >> Square_Start_XY
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> WB_block
  - >> GRAY_32
  - >> main
  - >> Load_Drow_Dialog
  - >> LT738_MakeTable
  - >> LT738_DrawQuadrangular
  - >> LT738_DrawCylinder
  - >> LT738_DrawSquare_Width
  - >> Show

  LT738_DrawSquare_Width (Thumb, 78 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawSquare_Fill
  [Called By]
  - >> LT738_MakeTable

  LT738_DrawCircleSquare (Thumb, 64 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Circle_Square_Radius_RxRy
  - >> Start_Circle_Square
  - >> Square_End_XY
  - >> Square_Start_XY

  LT738_DrawCircleSquare_Fill (Thumb, 64 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Circle_Square_Radius_RxRy
  - >> Start_Circle_Square_Fill
  - >> Square_End_XY
  - >> Square_Start_XY
  [Called By]
  - >> LT738_DrawCircleSquare_Width

  LT738_DrawCircleSquare_Width (Thumb, 86 bytes, Stack size 48 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawCircleSquare_Fill

  LT738_DrawTriangle (Thumb, 64 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  - >> Start_Triangle
  [Called By]
  - >> LT738_DrawTriangle_Frame

  LT738_DrawTriangle_Fill (Thumb, 100 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  - >> Start_Triangle_Fill
  [Called By]
  - >> LT738_DrawTriangle_Frame

  LT738_DrawTriangle_Frame (Thumb, 54 bytes, Stack size 48 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawTriangle_Fill
  - >> LT738_DrawTriangle

  LT738_DrawLeftUpCurve (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Left_Up_Curve
  [Called By]
  - >> LT738_SelectDrawCurve

  LT738_DrawLeftDownCurve (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Left_Down_Curve
  [Called By]
  - >> LT738_SelectDrawCurve

  LT738_DrawRightUpCurve (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Right_Up_Curve
  [Called By]
  - >> LT738_SelectDrawCurve

  LT738_DrawRightDownCurve (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Right_Down_Curve
  [Called By]
  - >> LT738_SelectDrawCurve

  LT738_SelectDrawCurve (Thumb, 114 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawRightDownCurve
  - >> LT738_DrawRightUpCurve
  - >> LT738_DrawLeftDownCurve
  - >> LT738_DrawLeftUpCurve

  LT738_DrawLeftUpCurve_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Left_Up_Curve_Fill
  [Called By]
  - >> LT738_SelectDrawCurve_Fill

  LT738_DrawLeftDownCurve_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Left_Down_Curve_Fill
  [Called By]
  - >> LT738_SelectDrawCurve_Fill

  LT738_DrawRightUpCurve_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Right_Up_Curve_Fill
  [Called By]
  - >> LT738_SelectDrawCurve_Fill

  LT738_DrawRightDownCurve_Fill (Thumb, 52 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_2D_Busy
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Start_Right_Down_Curve_Fill
  [Called By]
  - >> LT738_SelectDrawCurve_Fill

  LT738_SelectDrawCurve_Fill (Thumb, 114 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawRightDownCurve_Fill
  - >> LT738_DrawRightUpCurve_Fill
  - >> LT738_DrawLeftDownCurve_Fill
  - >> LT738_DrawLeftUpCurve_Fill

  LT738_DrawQuadrilateral (Thumb, 88 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> Check_2D_Busy
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  [Called By]
  - >> LT738_DrawQuadrangular

  LT738_DrawQuadrilateral_Fill (Thumb, 88 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> Check_2D_Busy
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY
  [Called By]
  - >> LT738_DrawQuadrangular

  LT738_DrawPentagon (Thumb, 92 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> Check_2D_Busy
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY

  LT738_DrawPentagon_Fill (Thumb, 92 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Busy_Draw
  - >> Check_2D_Busy
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Foreground_color_65k
  - >> Ellipse_Radius_RxRy
  - >> Ellipse_Center_XY
  - >> Triangle_Point3_XY
  - >> Triangle_Point2_XY
  - >> Triangle_Point1_XY

  LT738_DrawCylinder (Thumb, 166 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawLine
  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawEllipse_Fill
  - >> LT738_DrawEllipse

  LT738_DrawQuadrangular (Thumb, 130 bytes, Stack size 72 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare
  - >> LT738_DrawQuadrilateral_Fill
  - >> LT738_DrawQuadrilateral

  LT738_MakeTable (Thumb, 194 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> LT738_DrawSquare_Fill
  - >> LT738_DrawSquare_Width
  - >> LT738_DrawLine_Width

  LT738_Color_Bar_ON (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Color_Bar_ON

  LT738_Color_Bar_OFF (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Color_Bar_OFF

  LT738_Select_Internal_Font_Init (Thumb, 142 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LT738_Select_Internal_Font_Init ⇒ Font_Height_X4 ⇒ LCD_DataWrite
  [Calls]
  - >> Font_Height_X4
  - >> Font_Height_X3
  - >> Font_Height_X2
  - >> Font_Height_X1
  - >> Font_Width_X4
  - >> Font_Width_X3
  - >> Font_Width_X2
  - >> Font_Width_X1
  - >> Font_Background_select_Color
  - >> Font_Background_select_Transparency
  - >> Disable_Font_Alignment
  - >> Enable_Font_Alignment
  - >> Font_Select_16x32_32x32
  - >> Font_Select_12x24_24x24
  - >> Font_Select_8x16_16x16
  [Called By]
  - >> main
  - >> Load_Drow_Dialog

  LT738_Print_Internal_Font_String (Thumb, 54 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = LT738_Print_Internal_Font_String ⇒ Goto_Text_XY ⇒ LCD_RegisterWrite ⇒ LCD_DataWrite
  [Calls]
  - >> Text_Mode
  - >> Show_String
  - >> Background_color_65k
  - >> Foreground_color_65k
  - >> CGROM_Select_Internal_CGROM
  - >> Goto_Text_XY
  [Called By]
  - >> TP_Adjust
  - >> TP_Adj_Info_Show
  - >> main
  - >> Load_Drow_Dialog

  LT738_Print_Outside_Font_String (Thumb, 166 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Text_Mode
  - >> Graphic_Mode
  - >> Check_2D_Busy
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Background_color_65k
  - >> Foreground_color_65k
  - >> CGROM_Select_Internal_CGROM
  - >> Font_Select_UserDefine_Mode
  - >> Goto_Text_XY

  LT738_BTE_Memory_Copy_ColorExpansion_8 (Thumb, 116 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Background_color_256
  - >> Foreground_color_256
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_8bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_Memory_Copy_ColorExpansion_Chroma_key_8 (Thumb, 112 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Foreground_color_256
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_8bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_Text_cursor_Init (Thumb, 48 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Text_Cursor_H_V
  - >> Blinking_Time_Frames
  - >> Disable_Text_Cursor_Blinking
  - >> Enable_Text_Cursor_Blinking
  - >> Enable_Text_Cursor

  LT738_Enable_Text_Cursor (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Enable_Text_Cursor

  LT738_Disable_Text_Cursor (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Disable_Text_Cursor

  LT738_Graphic_cursor_Init (Thumb, 126 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Memory_Select_Graphic_Cursor_RAM
  - >> Memory_Select_SDRAM
  - >> Graphic_Mode
  - >> LCD_DataWrite
  - >> LCD_CmdWrite
  - >> Set_Graphic_Cursor_Color_2
  - >> Set_Graphic_Cursor_Color_1
  - >> Graphic_Cursor_XY
  - >> Select_Graphic_Cursor_4
  - >> Select_Graphic_Cursor_3
  - >> Select_Graphic_Cursor_2
  - >> Select_Graphic_Cursor_1
  - >> Enable_Graphic_Cursor

  LT738_Set_Graphic_cursor_Pos (Thumb, 64 bytes, Stack size 16 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Cursor_XY
  - >> Select_Graphic_Cursor_4
  - >> Select_Graphic_Cursor_3
  - >> Select_Graphic_Cursor_2
  - >> Select_Graphic_Cursor_1

  LT738_Enable_Graphic_Cursor (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Enable_Graphic_Cursor

  LT738_Disable_Graphic_Cursor (Thumb, 8 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Disable_Graphic_Cursor

  LT738_PIP_Init (Thumb, 124 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> PIP_Window_Image_Start_XY
  - >> PIP_Image_Width
  - >> PIP_Image_Start_Address
  - >> PIP_Display_Start_XY
  - >> Select_PIP1_Window_16bpp
  - >> Select_PIP2_Window_16bpp
  - >> Select_PIP2_Parameter
  - >> Select_PIP1_Parameter
  - >> Disable_PIP2
  - >> Enable_PIP2
  - >> Disable_PIP1
  - >> Enable_PIP1
  - >> PIP_Window_Width_Height

  LT738_Set_DisWindowPos (Thumb, 78 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> PIP_Display_Start_XY
  - >> Select_PIP2_Parameter
  - >> Select_PIP1_Parameter
  - >> Disable_PIP2
  - >> Enable_PIP2
  - >> Disable_PIP1
  - >> Enable_PIP1

  BTE_Solid_Fill (Thumb, 76 bytes, Stack size 32 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Foreground_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Operation_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_Memory_Copy (Thumb, 130 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S1_Window_Start_XY
  - >> BTE_S1_Image_Width
  - >> BTE_S1_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_Memory_Copy_Chroma_key (Thumb, 106 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Background_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_Pattern_Fill (Thumb, 116 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Pattern_Format_16X16
  - >> Pattern_Format_8X8
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_Pattern_Fill_With_Chroma_key (Thumb, 128 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Background_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Pattern_Format_16X16
  - >> Pattern_Format_8X8
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_MCU_Write_MCU_16bit (Thumb, 164 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S1_Window_Start_XY
  - >> BTE_S1_Image_Width
  - >> BTE_S1_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_MCU_Write_Chroma_key_MCU_16bit (Thumb, 132 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Background_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_MCU_Write_ColorExpansion_MCU_16bit (Thumb, 164 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> RGB_16b_16bpp
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Background_color_65k
  - >> Foreground_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_BTE_MCU_Write_ColorExpansion_Chroma_key_MCU_16bit (Thumb, 156 bytes, Stack size 56 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> RGB_16b_16bpp
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Foreground_color_65k
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_Operation_Code
  - >> BTE_ROP_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  BTE_Alpha_Blending (Thumb, 124 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> BTE_Alpha_Blending_Effect
  - >> BTE_Window_Size
  - >> BTE_Destination_Window_Start_XY
  - >> BTE_Destination_Image_Width
  - >> BTE_Destination_Memory_Start_Address
  - >> BTE_S1_Window_Start_XY
  - >> BTE_S1_Image_Width
  - >> BTE_S1_Memory_Start_Address
  - >> BTE_S0_Window_Start_XY
  - >> BTE_S0_Image_Width
  - >> BTE_S0_Memory_Start_Address
  - >> BTE_Destination_Color_16bpp
  - >> BTE_S1_Color_16bpp
  - >> BTE_S0_Color_16bpp
  - >> BTE_Operation_Code
  - >> Check_BTE_Busy
  - >> BTE_Enable

  LT738_PWM0_Init (Thumb, 86 bytes, Stack size 24 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Set_Timer0_Count_Buffer
  - >> Set_Timer0_Compare_Buffer
  - >> Stop_PWM0
  - >> Start_PWM0
  - >> Select_PWM0
  - >> Select_PWM0_Clock_Divided_By_8
  - >> Select_PWM0_Clock_Divided_By_4
  - >> Select_PWM0_Clock_Divided_By_2
  - >> Select_PWM0_Clock_Divided_By_1
  - >> Set_PWM_Prescaler_1_to_256

  LT738_PWM0_Duty (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Set_Timer0_Compare_Buffer

  LT738_PWM1_Init (Thumb, 86 bytes, Stack size 24 bytes, lt738_lib.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LT738_PWM1_Init ⇒ Set_Timer1_Count_Buffer ⇒ LCD_DataWrite
  [Calls]
  - >> Set_Timer1_Count_Buffer
  - >> Set_Timer1_Compare_Buffer
  - >> Stop_PWM1
  - >> Start_PWM1
  - >> Select_PWM1
  - >> Select_PWM1_Clock_Divided_By_8
  - >> Select_PWM1_Clock_Divided_By_4
  - >> Select_PWM1_Clock_Divided_By_2
  - >> Select_PWM1_Clock_Divided_By_1
  - >> Set_PWM_Prescaler_1_to_256
  [Called By]
  - >> main

  LT738_PWM1_Duty (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Set_Timer1_Compare_Buffer

  LT738_Standby (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Saving
  - >> Power_Saving_Standby_Mode

  LT738_Wkup_Standby (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Normal
  - >> Power_Normal_Mode

  LT738_Suspend (Thumb, 18 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Saving
  - >> LT738_SDRAM_initail
  - >> Power_Saving_Suspend_Mode

  LT738_Wkup_Suspend (Thumb, 20 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Normal
  - >> LT738_SDRAM_initail
  - >> Power_Normal_Mode

  LT738_SleepMode (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Saving
  - >> Power_Saving_Sleep_Mode

  LT738_Wkup_Sleep (Thumb, 12 bytes, Stack size 8 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Check_Power_is_Normal
  - >> Power_Normal_Mode

  MPU_Memory_Write_Window_8bit (Thumb, 148 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> Check_Mem_WR_FIFO_not_Full
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Active_Window_XY
  - >> Active_Window_WH
  - >> Goto_Pixel_XY

  MPU_Memory_Write_Pixel_8bit (Thumb, 94 bytes, Stack size 40 bytes, lt738_lib.o(.text), UNUSED)
  [Calls]

  - >> Graphic_Mode
  - >> Check_Mem_WR_FIFO_Empty
  - >> LCD_DataWrite_Pixel
  - >> LCD_CmdWrite
  - >> Goto_Pixel_XY

  GT9147_WR_Reg (Thumb, 92 bytes, Stack size 24 bytes, gt9147.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = GT9147_WR_Reg ⇒ CT_IIC_Send_Byte ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  [Called By]
  - >> GT9147_Scan
  - >> GT9147_Init
  - >> GT9147_Send_Cfg

  GT9147_Send_Cfg (Thumb, 80 bytes, Stack size 16 bytes, gt9147.o(.text), UNUSED)
  [Calls]

  - >> __2printf
  - >> GT9147_WR_Reg

  GT9147_RD_Reg (Thumb, 98 bytes, Stack size 24 bytes, gt9147.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = GT9147_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck ⇒ CT_Delay
  [Calls]
  - >> CT_IIC_Read_Byte
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  [Called By]
  - >> GT9147_Scan
  - >> GT9147_Init

  GT9147_Init (Thumb, 246 bytes, Stack size 264 bytes, gt9147.o(.text))
  [Stack]

  - Max Depth = 408 + Unknown Stack Size
  - Call Chain = GT9147_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> CT_IIC_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> delay_ms
  - >> __2printf
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg
  - >> strcmp
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  GT9147_Scan (Thumb, 516 bytes, Stack size 32 bytes, gt9147.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = GT9147_Scan ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  - >> GT9147_RD_Reg
  - >> GT9147_WR_Reg
  [Called By]
  - >> ctp_test

  delay_init (Thumb, 52 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> TP_Read_AD
  - >> TP_Write_Byte
  - >> CT_IIC_Read_Byte
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_Delay
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start

  delay_xms (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> delay_ms

  delay_ms (Thumb, 56 bytes, Stack size 16 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = delay_ms
  [Calls]
  - >> delay_xms
  [Called By]
  - >> TP_Adjust
  - >> AT24CXX_WriteOneByte
  - >> KEY_Scan
  - >> Scan_FunctionKey
  - >> Scan_Key_delay
  - >> WaitKeyBL
  - >> Scan_Key
  - >> WaitKey
  - >> GT9147_Init
  - >> main
  - >> ctp_test

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 22 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  uart_init (Thumb, 164 bytes, Stack size 40 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 122 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f40_41xxx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> main

  NVIC_Init (Thumb, 106 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  GPIO_DeInit (Thumb, 268 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> TP_Init
  - >> CT_IIC_Init
  - >> IIC_Init
  - >> FSMC_IO_Init
  - >> uart_init
  - >> LED_Init
  - >> KEY_Init
  - >> GT9147_Init
  - >> LT738_HW_Reset

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> KEY_Scan
  - >> Scan_FunctionKey
  - >> WaitKeyBL
  - >> Scan_Key
  - >> WaitKey

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> LED_Init
  - >> LT738_HW_Reset

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> LT738_HW_Reset

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> FSMC_IO_Init
  - >> uart_init

  FSMC_NORSRAMDeInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMInit (Thumb, 230 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text))
  [Called By]

  - >> FSMC_IO_Init

  FSMC_NORSRAMStructInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMCmd (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text))
  [Called By]

  - >> FSMC_IO_Init

  FSMC_NANDDeInit (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDInit (Thumb, 132 bytes, Stack size 12 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDStructInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDCmd (Thumb, 86 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDECCCmd (Thumb, 86 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetECC (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDDeInit (Thumb, 36 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDInit (Thumb, 130 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDCmd (Thumb, 44 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ITConfig (Thumb, 128 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetFlagStatus (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearFlag (Thumb, 74 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetITStatus (Thumb, 62 bytes, Stack size 16 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearITPendingBit (Thumb, 66 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  RCC_DeInit (Thumb, 82 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 222 bytes, Stack size 20 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_RTCCLKConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TP_Init
  - >> CT_IIC_Init
  - >> IIC_Init
  - >> FSMC_IO_Init
  - >> uart_init
  - >> LED_Init
  - >> KEY_Init
  - >> GT9147_Init
  - >> LT738_HW_Reset

  RCC_AHB2PeriphClockCmd (Thumb, 78 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> FSMC_IO_Init

  RCC_APB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> uart_init

  RCC_AHB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 206 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  USART_Init (Thumb, 204 bytes, Stack size 48 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 118 bytes, Stack size 16 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> test_FSMCIO
  - >> GT9147_Scan
  - >> GT9147_Init
  - >> GT9147_Send_Cfg

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_str
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  _printf_int_hex (Thumb, 84 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __printf (Thumb, 308 bytes, Stack size 40 bytes, __printf_flags_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> GT9147_Init

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> GT9147_Init

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> __hardfp_sqrt

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text), UNUSED)
  [Calls]

  - >> _printf_cs_common

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __hardfp_sqrt (Thumb, 122 bytes, Stack size 32 bytes, sqrt.o(i.__hardfp_sqrt))
  [Stack]

  - Max Depth = 72
  - Call Chain = __hardfp_sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  __aeabi_dneg (Thumb, 0 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)
  [Called By]

  - >> LT738_DrawLine_Width

  _dneg (Thumb, 6 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)

  __aeabi_fneg (Thumb, 0 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)

  _fneg (Thumb, 6 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)

  _dabs (Thumb, 6 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)

  _fabs (Thumb, 6 bytes, Stack size 0 bytes, basic.o(x$fpl$basic), UNUSED)

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_ddiv (Thumb, 0 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv), UNUSED)
  [Called By]

  - >> LT738_DrawLine_Width

  _ddiv (Thumb, 552 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> TP_Adjust

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)
  [Called By]

  - >> LT738_DrawLine_Width

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> TP_Adjust

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> TP_Adjust
  - >> LT738_DrawLine_Width

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> TP_Adjust

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dsqrt
  - >> _dmul
  - >> _dcmple
  - >> _dfixu
  - >> _ddiv

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d
  - >> _dmul
  - >> _ddiv

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> TP_Adjust
  - >> LT738_DrawLine_Width

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  _dsqrt (Thumb, 404 bytes, Stack size 24 bytes, dsqrt_umaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> __hardfp_sqrt

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> TP_Adjust

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _f2d

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 220 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols