6.0.2 Record page
Descri
ption
The top row of data from left to right are boot record time and onboard
temperature respectively;
The uppercase data on the left is voltage, current, and power from top to
bottom;
The curve and progress bar on the right are the remaining storage
capacity of the voltage and current curves;
The groups on the right are from top to bottom,statistics group,
current group capacity, power, time value;
Starting from the lower left corner, the Min, Max, and Avg data are the minimum,
maximum, and average values of voltage, current, and power respectively. Voltage,
current, and power can be distinguished according to the unit;
There are two text boxes in the lower right corner, the first 1.0 from top
to bottom is the setting menu -> recording -> offline recording time, in
hours, it is highlighted when recording, otherwise it is grayed out; the
second is the setting menu -> Record->Energy statistics time, unit hour,
when the value is 0.0, it means there is no time limit for statistics.
Instructions
(1) Long press the left button: switch to the capacity/power consumption list (please see
the following instructions).
(2) Click the middle button: start/stop the voltage and current curve recording, it cannot
be started when the recording time is 0.
(3) Long press the middle button: restart the calculation of the minimum, maximum and
average values of voltage, current and power.
(4) Long press the right button: enter the battery capacity calculation tool (please see the
subsequent instructions).
12