# Adafruit_FT6206 Library [![Build Status](https://github.com/adafruit/Adafruit_FT6206_Library/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_FT6206_Library/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_FT6206_Library/html/index.html)

<img src="https://cdn-shop.adafruit.com/970x728/1947-05.jpg" height="300"/>

This is a library for the Adafruit FT6206-Based capacitive touch screens and displays:
  * https://www.adafruit.com/products/1947
  * https://www.adafruit.com/product/1651

Also supports FT6236 chips (and maybe other compatible chips!)
 
Check out the links above for our tutorials and wiring diagrams. This chip uses I2C to communicate

Adafruit invests time and resources providing this open source code, please support Adafruit and open-source hardware by purchasing products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.
MIT license, all text above must be included in any redistribution

